**Bibliography**

Abousleiman, Y., Tran, M., Hoang, S., Bobko, C., Ortega, A., Ulm, F.J., 2007. Geomechanics field and laboratory characterization of woodford shale: The next gas play. Proceedings - SPE Annual Technical Conference and Exhibition 4, 2127–2140. <https://doi.org/10.2523/110120-ms>

Ader, T., Chendorain, M., Free, M., Saarno, T., Heikkinen, P., Malin, P.E., Leary, P., Kwiatek, G., Dresen, G., Bluemle, F. and Vuorinen, T., 2020. Design and implementation of a traffic light system for deep geothermal well stimulation in Finland. Journal of seismology, 24(5), pp.991-1014. <https://doi.org/10.1007/s10950-019-09853-y>

Ake, J., Mahrer, K., O’Connell, D. and Block, L., 2005. Deep-injection and closely monitored induced seismicity at Paradox Valley, Colorado. Bulletin of the Seismological Society of America, 95(2), pp.664-683. <https://doi.org/10.1785/0120040072>

Albaric, J., Oye, V., Hasting, M., Messeiller, M. and Reid, P., 2013, March. Induced seismicity patterns in the Paralana geothermal reservoir, South Australia. In 4th EAGE Passive Seismic Workshop (pp. cp-337). European Association of Geoscientists & Engineers. <https://doi.org/10.3997/2214-4609.20142349>

Albaric, J., Oye, V., Langet, N., Hasting, M., Lecomte, I., Iranpour, K., Messeiller, M. and Reid, P., 2014. Monitoring of induced seismicity during the first geothermal reservoir stimulation at Paralana, Australia. Geothermics, 52, pp.120-131. <https://doi.org/10.1016/j.geothermics.2013.10.013>

Anderson, I., Ma, J., Wu, X., Stow, D. and Underhill, J.R., 2019, July. Assessing the stratigraphic variations in geomechanical properties of the United Kingdom Bowland Shale using wireline and seismic data: How could these guide the placement of lateral wells?. In SPE/AAPG/SEG Unconventional Resources Technology Conference. OnePetro. <https://doi.org/10.15530/urtec-2019-257>

Andres, S., Santillan, D., Mosquera, J.C. and Cueto-Felgueroso, L., 2019. Thermo-Poroelastic Analysis of Induced Seismicity at the Basel Enhanced Geothermal System. Sustainability, 11(24), p.6904. <https://doi.org/10.3390/su11246904>

Arnórsson, S., 1995. Geothermal systems in Iceland: structure and conceptual models—I. High-temperature areas. Geothermics, 24(5-6), pp.561-602. <https://doi.org/10.1016/0375-6505(95)00025-9>

Arzate, J., Corbo-Camargo, F., Carrasco-Núñez, G., Hernández, J. and Yutsis, V., 2018. The Los Humeros (Mexico) geothermal field model deduced from new geophysical and geological data. Geothermics, 71, pp.200-211. <https://doi.org/10.1016/j.geothermics.2017.09.009>

Asanuma, H., Soma, N., Kaieda, H., Kumano, Y., Izumi, T., Tezuka, K., Niitsuma, H. and Wyborn, D., 2005, April. Microseismic monitoring of hydraulic stimulation at the Australian HDR project in Cooper Basin. In Proceedings World Geothermal Congress (pp. 24-29).

Atkinson, G.M., Eaton, D.W., Ghofrani, H., Walker, D., Cheadle, B., Schultz, R., Shcherbakov, R., Tiampo, K., Gu, J., Harrington, R.M. and Liu, Y., 2016. Hydraulic fracturing and seismicity in the Western Canada Sedimentary Basin. Seismological research letters, 87(3), pp.631-647. <https://doi.org/10.1785/0220150263>

Audigane, P., Royer, J.J. and Kaieda, H., 2002. Permeability characterization of the Soultz and Ogachi large-scale reservoir using induced microseismicity. Geophysics, 67(1), pp.204-211. <https://doi.org/10.1190/1.1451573>

Axelsson, G., Björnsson, G., Egilson, T., Flóvenz, Ó.G., Gautason, B., Hauksdóttir, S., Ólafsson, M., Smárason, Ó.B. and Sæmundsson, K., 2005, April. Nature and properties of recently discovered hidden low-temperature geothermal reservoirs in Iceland. In World Geothermal Congress (pp. 24-29).

Axelsson, G., Gunnlaugsson, E., Jónasson, T. and Ólafsson, M., 2010. Low-temperature geothermal utilization in Iceland–Decades of experience. Geothermics, 39(4), pp.329-338. <https://doi.org/10.1016/j.geothermics.2010.09.002>

Bachmann, C.E., Wiemer, S., Woessner, J. and Hainzl, S., 2011. Statistical analysis of the induced Basel 2006 earthquake sequence: introducing a probability-based monitoring approach for Enhanced Geothermal Systems. Geophysical Journal International, 186(2), pp.793-807. <https://doi.org/10.1111/j.1365-246X.2011.05068.x>

Baisch, S. and Harjes, H.P., 2003. A model for fluid-injection-induced seismicity at the KTB, Germany. Geophysical Journal International, 152(1), pp.160-170. <https://doi.org/10.1046/j.1365-246X.2003.01837.x>

Baisch, S., Rothert, E., Stang, H., Vörös, R., Koch, C. and McMahon, A., 2015. Continued geothermal reservoir stimulation experiments in the Cooper Basin (Australia). Bulletin of the Seismological Society of America, 105(1), pp.198-209. <https://doi.org/10.1785/0120140208>

Baisch, S., Vörös, R., Rothert, E., Stang, H., Jung, R. and Schellschmidt, R., 2010. A numerical model for fluid injection induced seismicity at Soultz-sous-Forêts. International Journal of Rock Mechanics and Mining Sciences, 47(3), pp.405-413. <https://doi.org/10.1016/j.ijrmms.2009.10.001>

Baisch, S., Vörös, R., Weidler, R. and Wyborn, D., 2009. Investigation of fault mechanisms during geothermal reservoir stimulation experiments in the Cooper Basin, Australia. Bulletin of the Seismological Society of America, 99(1), pp.148-158. <https://doi.org/10.1785/0120080055>

Baisch, S., Weidler, R., Vörös, R., Wyborn, D. and de Graaf, L., 2006. Induced seismicity during the stimulation of a geothermal HFR reservoir in the Cooper Basin, Australia. Bulletin of the Seismological Society of America, 96(6), pp.2242-2256. <https://doi.org/10.1785/0120050255>

Bao, X. and Eaton, D.W., 2016. Fault activation by hydraulic fracturing in western Canada. science, 354(6318), pp.1406-1409. 10.1126/science.aag2583

Barbour, A.J., Norbeck, J.H. and Rubinstein, J.L., 2017. The effects of varying injection rates in Osage County, Oklahoma, on the 2016 M w 5.8 Pawnee earthquake. Seismological Research Letters, 88(4), pp.1040-1053. <https://doi.org/10.1785/0220170003>

Barelli, A., Ceccarelli, A., Dini, I., Fiordelisi, A., Giorgi, N., Lovari, F. and Romagnoli, P., 2010, April. A review of the Mt. Amiata geothermal system (Italy). In Proceedings world geothermal congress (Vol. 2010, pp. 1-4).

Barnhart, W.D., Benz, H.M., Hayes, G.P., Rubinstein, J.L. and Bergman, E., 2014. Seismological and geodetic constraints on the 2011 Mw5. 3 Trinidad, Colorado earthquake and induced deformation in the Raton Basin. Journal of Geophysical Research: Solid Earth, 119(10), pp.7923-7933. <https://doi.org/10.1002/2014JB011227>

Barton, C.A., Moos, D., Hartley, L., Baxter, S., Foulquier, L., Holl, H., Hogarth, R. and Brisbane, A., 2013, February. Geomechanically coupled simulation of flow in fractured reservoirs. In Proceedings 38th Workshop on Geothermal Reservoir Engineering, Stanford University, Stanford, California, February (pp. 11-13).

Batchelor, A.S., Baria, R. and Hearn, K., 1983, October. Monitoring the effects of hydraulic stimulation by microseismic event location: a case study. In SPE Annual Technical Conference and Exhibition. OnePetro. <https://doi.org/10.2118/12109-MS>

Batchelor, J.A., Sherley, B., Klepacki, D., Lewis, R. and Jensen, R.E., 2007, September. Validating the integrity of the Amposta structure for gas storage offshore Spain. In SPE Offshore Europe Oil and Gas Conference and Exhibition. OnePetro. <https://doi.org/10.2118/108247-MS>

Batir, J., Davatzes, N.C. and Asmundsson, R., 2012. Preliminary model of fracture and stress state in the Hellisheidi Geothermal Field, Hengill Volcanic System, Iceland. In Proceedings of the Thirty-Seventh Workshop on Geothermal Reservoir Engineering, Stanford.

Bauer, R.A., Carney, M. and Finley, R.J., 2016. Overview of microseismic response to CO2 injection into the Mt. Simon saline reservoir at the Illinois Basin-Decatur Project. International Journal of Greenhouse Gas Control, 54, pp.378-388. <https://doi.org/10.1016/j.ijggc.2015.12.015>

BC Oil and Gas Commision:Investigation of Observed Seismicity in the Horn River Basin, 2012.

BC Oil and Gas Commission: Investigation of Observed Seismicity in the Montney Trend, 2014.

Belitz, K. and Bredehoeft, J.D., 1988. Hydrodynamics of Denver Basin: Explanation of subnormal fluid pressures. AAPG bulletin, 72(11), pp.1334-1359. <https://doi.org/10.1306/703C999C-1707-11D7-8645000102C1865D>

Benato, S., Hickman, S., Davatzes, N.C., Taron, J., Spielman, P., Elsworth, D., Majer, E.L. and Boyle, K., 2016. Conceptual model and numerical analysis of the Desert Peak EGS project: Reservoir response to the shallow medium flow-rate hydraulic stimulation phase. Geothermics, 63, pp.139-156. <https://doi.org/10.1016/j.geothermics.2015.06.008>

Bentz, S., Kwiatek, G., Martínez‐Garzón, P., Bohnhoff, M. and Dresen, G., 2020. Seismic moment evolution during hydraulic stimulations. Geophysical Research Letters, 47(5), p.e2019GL086185. <https://doi.org/10.1029/2019GL086185>

Benz, H.M., McMahon, N.D., Aster, R.C., McNamara, D.E. and Harris, D.B., 2015. Hundreds of earthquakes per day: The 2014 Guthrie, Oklahoma, earthquake sequence. Seismological Research Letters, 86(5), pp.1318-1325. <https://doi.org/10.1785/0220150019>

Birkholzer, J.T., Guglielmi, Y. and Jeanne, P., 2016. Results from the In Situ Fault Slip Experiment at Mont Terri.

Bjornsson, G., 2004, January. Reservoir conditions at 3-6 km depth in the Hellisheidi geothermal field, SW-Iceland, estimated by deep drilling, cold water injection and seismic monitoring. In Proceedings (pp. 26-28).

Björnsson, G., Flovenz, Ó.G., Saemundsson, K. and Einarsson, E.M., 2001, January. Pressure changes in Icelandic geothermal reservoirs associated with two large earthquakes in June 2000. In Proceedings of the 26th Workshop on Geothermal Reservoir Engineering, Stanford University, Stanford, California.

Blöcher, G., Cacace, M., Jacquey, A. B., Zang, A., Heidbach, O., Hofmann, H., Kluge, C., and Zimmermann, G., 2018. Evaluating micro-seismic events triggered by reservoir operations at the geothermal site of Groß Schönebeck (Germany). Rock Mechanics and Rock Engineering, 51(10), pp.3265-3279. <https://doi.org/10.1007/s00603-018-1521-2>

Bommer, J.J., Oates, S., Cepeda, J.M., Lindholm, C., Bird, J., Torres, R., Marroquín, G. and Rivas, J., 2006. Control of hazard due to seismicity induced by a hot fractured rock geothermal project. Engineering geology, 83(4), pp.287-306. <https://doi.org/10.1016/j.enggeo.2005.11.002>

Boyle, K. and Zoback, M., 2014. The stress state of the Northwest Geysers, California geothermal field, and implications for fault‐controlled fluid flow. Bulletin of the Seismological Society of America, 104(5), pp.2303-2312. <https://doi.org/10.1785/0120130284>

Braun, T., Cesca, S., Kühn, D., Martirosian-Janssen, A. and Dahm, T., 2018. Anthropogenic seismicity in Italy and its relation to tectonics: state of the art and perspectives. Anthropocene, 21, pp.80-94. <https://doi.org/10.1016/j.ancene.2018.02.001>

Breede, K., Dzebisashvili, K., Liu, X., and Falcone, G., 2013. A systematic review of enhanced (or engineered) geothermal systems: past, present and future. Geothermal Energy, 1(1), pp.1-27. <https://doi.org/10.1186/2195-9706-1-4>

Brinkley, S.A., 2016. Petroleum Geology of the Utica/Point Pleasant Play in Washington County, Ohio.

Broothaers, M., Bos, S., Lagrou, D., Harcouët-Menou, V., and Laenen, B.: Lower Carboniferous limestone reservoir in northern Belgium: structural insights from the Balmatt project in Mol, in: Proceedings European Geothermal Congress, The Hague, 2019.

Brudy, M., Zoback, M.D., Fuchs, K., Rummel, F. and Baumgärtner, J., 1997. Estimation of the complete stress tensor to 8 km depth in the KTB scientific drill holes: Implications for crustal strength. Journal of Geophysical Research: Solid Earth, 102(B8), pp.18453-18475. <https://doi.org/10.1029/96JB02942>

Brudy, M., Zoback, M.D., Rummel, F. and Fuchs, K., 1995. Application of the integrated stress measurement strategy to the 9 km depth in the KTB boreholes. In Proc. Workshop on Rock Stresses in the North Sea (pp. 154-164). Trondheim, Norway: NTH and SINTEF Publ.

Brudzinski, M.R. and Kozłowska, M., 2019. Seismicity induced by hydraulic fracturing and wastewater disposal in the Appalachian Basin, USA: A review. Acta Geophysica, 67(1), pp.351-364. <https://doi.org/10.1007/s11600-019-00249-7>

Buijze, L., van Bijsterveldt, L., Cremer, H., Paap, B., Veldkamp, H., Wassing, B. B., van Wees, J.D., van Yperen, G.C., ter Heege, J.H., and Jaarsma, B., 2019. Review of induced seismicity in geothermal systems worldwide and implications for geothermal systems in the Netherlands. Netherlands Journal of Geosciences, pp.98. <https://doi.org/10.1029/2018JB016941>

Buttinelli, M., Improta, L., Bagh, S. and Chiarabba, C., 2016. Inversion of inherited thrusts by wastewater injection induced seismicity at the Val d’Agri oilfield (Italy). Scientific reports, 6(1), pp.1-8. <https://doi.org/10.1038/srep37165>

Cabral, E., 2018. Thermoeconomic analysis of EGS/Deep Geothermal Resources in the region of Alsace, France (Doctoral dissertation).

Calò, M., Dorbath, C. and Frogneux, M., 2014. Injection tests at the EGS reservoir of Soultz-sous-Forêts. Seismic response of the GPK4 stimulations. Geothermics, 52, pp.50-58. <https://doi.org/10.1016/j.geothermics.2013.10.007>

Cant, J.L., Siratovich, P.A., Cole, J.W., Villeneuve, M.C. and Kennedy, B.M., 2018. Matrix permeability of reservoir rocks, Ngatamariki geothermal field, Taupo volcanic zone, New Zealand. Geothermal Energy, 6(1), pp.1-28. <https://doi.org/10.1186/s40517-017-0088-6>

Cao, W., Durucan, S., Shi, J.Q., Cai, W., Korre, A. and Ratouis, T., 2022. Induced seismicity associated with geothermal fluids re-injection: Poroelastic stressing, thermoelastic stressing, or transient cooling-induced permeability enhancement?. Geothermics, 102, p.102404. <https://doi.org/10.1016/j.geothermics.2022.102404>

Cesca, S., Grigoli, F., Heimann, S., González, Á., Buforn, E., Maghsoudi, S., Blanch, E. and Dahm, T., 2014. The 2013 September–October seismic sequence offshore Spain: a case of seismicity triggered by gas injection?. Geophysical Journal International, 198(2), pp.941-953. <https://doi.org/10.1093/gji/ggu172>

Chalmers, G.R., Ross, D.J. and Bustin, R.M., 2012. Geological controls on matrix permeability of Devonian Gas Shales in the Horn River and Liard basins, northeastern British Columbia, Canada. International Journal of Coal Geology, 103, pp.120-131. <https://doi.org/10.1016/j.coal.2012.05.006>

Chang, C. and Haimson, B., 2000. True triaxial strength and deformability of the German Continental Deep Drilling Program (KTB) deep hole amphibolite. Journal of Geophysical Research: Solid Earth, 105(B8), pp.18999-19013. <https://doi.org/10.1029/2000JB900184>

Chen, X., Haffener, J., Goebel, T.H., Meng, X., Peng, Z. and Chang, J.C., 2018. Temporal correlation between seismic moment and injection volume for an induced earthquake sequence in central Oklahoma. Journal of Geophysical Research: Solid Earth, 123(4), pp.3047-3064. <https://doi.org/10.1002/2017JB014694>

Chen, X., Nakata, N., Pennington, C., Haffener, J., Chang, J. C., He, X., Zhan, Z., Ni, S., and Walter, J. I., 2017. The Pawnee earthquake as a result of the interplay among injection, faults and foreshocks. Scientific Reports, 7(1), pp.1-18. <https://doi.org/10.1038/s41598-017-04992-z>

Cheng, Q., Wang, X. and Ghassemi, A., 2019. Numerical simulation of reservoir stimulation with reference to the Newberry EGS. Geothermics, 77, pp.327-343. <https://doi.org/10.1016/j.geothermics.2018.09.011>

Cheng, W.Z., Chen, T.C. and Qiao, H.Z., 2003. Source parameters for the earthquake sequence of Rongchang M5.2 (in Chinese). Earthquake, 23(3), pp.79-88. <http://dizhen.ief.ac.cn/CN/Y2003/V23/I3/79>

Cladouhos, T.T., Petty, S., Nordin, Y., Moore, M., Grasso, K., Uddenberg, M., Swyer, M., Julian, B. and Foulger, G., 2013, February. Microseismic monitoring of Newberry volcano EGS demonstration. In Proceedings of the 38th Workshop on Geothermal Reservoir Engineering, Stanford, CA (pp. 11-13).

Cladouhos, T.T., Petty, S., Swyer, M.W., Uddenberg, M.E., Grasso, K. and Nordin, Y., 2016. Results from newberry volcano EGS demonstration, 2010–2014. Geothermics, 63, pp.44-61. <https://doi.org/10.1016/j.geothermics.2015.08.009>

Clarke, H., Eisner, L., Styles, P. and Turner, P., 2014. Felt seismicity associated with shale gas hydraulic fracturing: The first documented example in Europe. Geophysical Research Letters, 41(23), pp.8308-8314. <https://doi.org/10.1002/2014GL062047>

Clarke, H., Soroush, H. and Wood, T., 2019, June. Preston new road: the role of geomechanics in successful drilling of the UK's first horizontal shale gas well. In SPE Europec featured at 81st EAGE Conference and Exhibition. OnePetro. <https://doi.org/10.2118/195563-MS>

Clarke, H., Turner, P., Bustin, R.M., Riley, N. and Besly, B., 2018. Shale gas resources of the Bowland Basin, NW England: a holistic study. Petroleum Geoscience, 24(3), pp.287-322. <https://doi.org/10.1144/petgeo2017-066>

Clarke, H., Verdon, J.P., Kettlety, T., Baird, A.F. and Kendall, J.M., 2019. Real‐time imaging, forecasting, and management of human‐induced seismicity at Preston New Road, Lancashire, England. Seismological Research Letters, 90(5), pp.1902-1915. <https://doi.org/10.1785/0220190110>

Cluff, S.G., Cluff, R.M., 2004. Petrophysics of the Lance Sandstone Reservoirs in Jonah Field, Sublette County, Wyoming. Jonah Field: case study of a tight-gas fluvial reservoir. <https://doi.org/10.1306/St521007>

Columbia, B. and Oil and Gas Commission, 2012. Investigation of observed seismicity in the Horn River Basin. BC Oil and Gas Commission.

Columbia, B. and Oil and Gas Commission, 2014. Investigation of observed seismicity in the Montney Trend. BC Oil and Gas Commission.

Cornet, F.H., Helm, J., Poitrenaud, H. and Etchecopar, A., 1997. Seismic and aseismic slips induced by large-scale fluid injections. In Seismicity associated with mines, reservoirs and fluid injections (pp. 563-583). Birkhäuser, Basel. <https://doi.org/10.1007/978-3-0348-8814-1_12>

Cox, R.T., 1991. Possbile Triggering of Earthquakes by Underground Waste Disposal in the El Dorado, Arkansas Area. Seismological Research Letters, 62(2), pp.113-122. https://doi.org/10.1785/gssrl.62.2.113

Cuadrilla Resources, 2019. Preston New Road-1z: LJ/06-09 (z) HFP Report.

Cuenot, N., Charléty, J., Dorbath, L. and Haessler, H., 2006. Faulting mechanisms and stress regime at the European HDR site of Soultz-sous-Forêts, France. Geothermics, 35(5-6), pp.561-575. <https://doi.org/10.1016/j.geothermics.2006.11.007>

Damore, F. and Mejia, J.T., 1999. Chemical and physical reservoir parameters at initial conditions in Berlingeothermal field, El Salvador: a first assessment. Geothermics, 28(1), pp.45-73. <https://doi.org/10.1016/S0375-6505(98)00044-3>

Darold, A., Holland, A.A., Chen, C., Youngblood, A., 2014. Preliminary Analysis of Seismicity Near Eagleton 1-29, Carter County, July 2014.

Davatzes, N. C., and Hickman, S.: Stress and faulting in the Coso Geothermal Field: Update and recent results from the East Flank and Coso Wash, in: Proceedings of the 31st Workshop on Geothermal Reservoir Engineering, 13-19, January 2006.

Davatzes, N.C. and Hickman, S.H., 2009. Fractures, stress and fluid flow prior to stimulation of well 27-15, Desert Peak, Nevada, EGS Project. In Thirty-Fourth Workshop on Geothermal Reservoir Engineering.

Davey, H., 2012. Geomechanical characterization of the Montney Shale northwest Alberta and northeast British Columbia, Canada. Colorado School of Mines.

David, C., Wassermann, J., Amann, F., Klaver, J., Davy, C., Sarout, J., Esteban, L., Rutter, E.H., Hu, Q., Louis, L. and Delage, P., 2018. KG²B, a collaborative benchmarking exercise for estimating the permeability of the Grimsel granodiorite—Part 2: modelling, microstructures and complementary data. Geophysical Journal International, 215(2), pp.825-843. <https://doi.org/10.1093/gji/ggy305>

David, C., Wassermann, J., Amann, F., Lockner, D.A., Rutter, E.H., Vanorio, T., Amann Hildenbrand, A., Billiotte, J., Reuschlé, T., Lasseux, D. and Fortin, J., 2018. KG²B, a collaborative benchmarking exercise for estimating the permeability of the Grimsel granodiorite–Part 1: measurements, pressure dependence and pore-fluid effects. Geophysical Journal International, 215(2), pp.799-824. <https://doi.org/10.1093/gji/ggy304>

Davidson, J., Siratovich, P., Wallis, I., Gravley, D. and McNamara, D.D., 2012. Quantifying the stress distribution at the Rotokawa geothermal field, New Zealand. In New Zealand Geothermal Workshop 2012. New Zealand Geothermal Workshop.

Davies, R., Foulger, G., Bindley, A. and Styles, P., 2013. Induced seismicity and hydraulic fracturing for the recovery of hydrocarbons. Marine and petroleum geology, 45, pp.171-185. <https://doi.org/10.1016/j.marpetgeo.2013.03.016>

De Barros, L., Daniel, G., Guglielmi, Y., Rivet, D., Caron, H., Payre, X., Bergery, G., Henry, P., Castilla, R., Dick, P. and Barbieri, E., 2016. Fault structure, stress, or pressure control of the seismicity in shale? Insights from a controlled experiment of fluid‐induced fault reactivation. Journal of Geophysical Research: Solid Earth, 121(6), pp.4506-4522. <https://doi.org/10.1002/2015JB012633>

De Barros, L., Guglielmi, Y., Rivet, D., Cappa, F. and Duboeuf, L., 2018. Seismicity and fault aseismic deformation caused by fluid injection in decametric in-situ experiments. Comptes Rendus Geoscience, 350(8), pp.464-475. <https://doi.org/10.1016/j.crte.2018.08.002>

De Dios, J.C., Delgado, M.A., Martínez, C., Ramos, A., Álvarez, I., Marín, J.A. and Salvador, I., 2017. Hydraulic characterization of fractured carbonates for CO2 geological storage: Experiences and lessons learned in Hontomín Technology Development Plant. International Journal of Greenhouse Gas Control, 58, pp.185-200. <https://doi.org/10.1016/j.ijggc.2017.01.008>

De Pater, C.J. and Baisch, S., 2011. Geomechanical study of Bowland Shale seismicity. Synthesis report, 57.

Deichmann, N., Kraft, T. and Evans, K.F., 2014. Identification of faults activated during the stimulation of the Basel geothermal project from cluster analysis and focal mechanisms of the larger magnitude events. Geothermics, 52, pp.84-97. <http://dx.doi.org/10.1016/j.geothermics.2014.04.001>

Dempsey, D., Kelkar, S., Davatzes, N., Hickman, S. and Moos, D., 2015. Numerical modeling of injection, stress and permeability enhancement during shear stimulation at the Desert Peak Enhanced Geothermal System. International Journal of Rock Mechanics and Mining Sciences, 78, pp.190-206. <https://doi.org/10.1016/j.ijrmms.2015.06.003>

Dempsey, D., Suckale, J. and Huang, Y., 2016. Collective properties of injection‐induced earthquake sequences: 2. Spatiotemporal evolution and magnitude frequency distributions. Journal of Geophysical Research: Solid Earth, 121(5), pp.3638-3665. <https://doi.org/10.1002/2015JB012551>

Denllinger, M., Majer, E., Freeman, K., Johnson, L.R., Jarpe, S., Nihei, K. and Walters, M., 2017. Final report: Monitoring the effect of injection of fluids from the Lake County pipeline on seismicity at The Geysers, California, geothermal field, United States. United States.

Derode, B., Cappa, F., Guglielmi, Y. and Rutqvist, J., 2013. Coupled seismo-hydromechanical monitoring of inelastic effects on injection-induced fracture permeability. International Journal of Rock Mechanics and Mining Sciences, 61, pp.266-274. <https://doi.org/10.1016/j.ijrmms.2013.03.008>

Derode, B., Guglielmi, Y., De Barros, L. and Cappa, F., 2015. Seismic responses to fluid pressure perturbations in a slipping fault. Geophysical Research Letters, 42(9), pp.3197-3203. <https://doi.org/10.1002/2015GL063671>

Dewers, T., Newell, P., Broome, S., Heath, J. and Bauer, S., 2014. Geomechanical behavior of cambrian mount simon sandstone reservoir lithofacies, iowa shelf, USA. International Journal of Greenhouse Gas Control, 21, pp.33-48. <https://doi.org/10.1016/j.ijggc.2013.11.010>

Dong, T., 2016. Geochemical, petrophysical and geomechanical properties of stratigraphic sequences in Horn River Shale, Middle and Upper Devonian, northeastern British Columbia, Canada.

Dong, Tian. Geochemical, Petrophysical and Geomechanical Properties of Stratigraphic Sequences in Horn River Shale, Middle and Upper Devonian, Northeastern British Columbia, Canada. University of Alberta, 2016.

Dorbath, L., Cuenot, N., Genter, A. and Frogneux, M., 2009. Seismic response of the fractured and faulted granite of Soultz-sous-Forêts (France) to 5 km deep massive water injections. Geophysical Journal International, 177(2), pp.653-675. <https://doi.org/10.1111/j.1365-246X.2009.04030.x>

Duboeuf, L., De Barros, L., Cappa, F., Guglielmi, Y., Deschamps, A. and Seguy, S., 2017. Aseismic motions drive a sparse seismicity during fluid injections into a fractured zone in a carbonate reservoir. Journal of Geophysical Research: Solid Earth, 122(10), pp.8285-8304. <https://doi.org/10.1002/2017JB014535>

Duchane, D., and Brown, D., 2002. Hot dry rock (HDR) geothermal energy research and development at Fenton Hill, New Mexico. Geo-Heat Centre Quarterly Bulletin, pp.23.

Dutler, N., Valley, B., Gischig, V., Jalali, M., Brixel, B., Krietsch, H., Roques, C. and Amann, F., 2020. Hydromechanical insight of fracture opening and closure during in-situ hydraulic fracturing in crystalline rock. International Journal of Rock Mechanics and Mining Sciences, 135, p.104450. <https://doi.org/10.1016/j.ijrmms.2020.104450>

Eaton, D.W., Igonin, N., Poulin, A., Weir, R., Zhang, H., Pellegrino, S., Rodriguez, G., 2018. Induced seismicity characterization during hydraulic-fracture monitoring with a shallow-wellbore geophone array and broadband sensors. Seismological Research Letters 89, 1641–1651. <https://doi.org/10.1785/0220180055>

Eaton, D.W., Salvage, R., Kao, H. and van der Baan, M., 2019, October. A tale of three earthquakes: New insights into fault activation in light of recent occurrences in western Canada. In New Directions in Geosciences for Unconventional Resources Conference.

Eggertsson, G.H., 2019. Constraining mechanical and permeability properties of the Krafla geothermal reservoir, North-East Iceland. The University of Liverpool (United Kingdom).

Eggertsson, G.H., Lavallée, Y., Kendrick, J.E. and Markússon, S.H., 2020. Improving fluid flow in geothermal reservoirs by thermal and mechanical stimulation: The case of Krafla volcano, Iceland. Journal of Volcanology and Geothermal Research, 391, p.106351. <https://doi.org/10.1016/j.jvolgeores.2018.04.008>

Eliasson, T., 1993. Mineralogy, geochemistry and petrophysics of red coloured granite adjacent to fractures (No. SKB-TR--93-06). Swedish Nuclear Fuel and Waste Management Co.

Eliasson, T., Lindblom, U., Slunga, R., Sundqvist, U., and Wallroth, T., 1988. The Swedish Hot-Dry-Rock Project; Some Preliminary Achievements. In: Deep Drilling in Crystalline Bedrock, pp. 391-400. <https://doi.org/10.1007/978-3-642-73455-7_32>

Ellsworth, W.L., Giardini, D., Townend, J., Ge, S. and Shimamoto, T., 2019. Triggering of the Pohang, Korea, earthquake (M w 5.5) by enhanced geothermal system stimulation. Seismological Research Letters, 90(5), pp.1844-1858. <https://doi.org/10.1785/0220190102>

Erol, S., 2018. Reactive Transport Simulations of the Lower Carboniferous Limestone Geothermal Reservoir.

Evans, D.M., 1966. The Denver area earthquakes and the Rocky Mountain Arsenal disposal well. The Mountain Geologist.

Evans, K. F., Zappone, A., Kraft, T., Deichmann, N., and Moia, F., 2012. A survey of the induced seismic responses to fluid injection in geothermal and CO2 reservoirs in Europe. Geothermics, 41, pp.30-54. <https://doi.org/10.1016/j.geothermics.2011.08.002>

Evans, K.F., 2005. Permeability creation and damage due to massive fluid injections into granite at 3.5 km at Soultz: 2. Critical stress and fracture strength. Journal of Geophysical Research: Solid Earth, 110(B4). <https://doi.org/10.1029/2004JB003169>

Eyre, T.S., Eaton, D.W., Garagash, D.I., Zecevic, M., Venieri, M., Weir, R. and Lawton, D.C., 2019. The role of aseismic slip in hydraulic fracturing–induced seismicity. Science advances, 5(8), p.eaav7172. DOI: 10.1126/sciadv.aav7172

Fan, Z., Eichhubl, P. and Gale, J.F., 2016. Geomechanical analysis of fluid injection and seismic fault slip for the Mw4. 8 Timpson, Texas, earthquake sequence. Journal of Geophysical Research: Solid Earth, 121(4), pp.2798-2812. <https://doi.org/10.1002/2016JB012821>

Fehler, M. C.: Stress control of seismicity patterns observed during hydraulic fracturing experiments at the Fenton Hill hot dry rock geothermal energy site, New Mexico, in: International Journal of Rock Mechanics and Mining Sciences and Geomechanics Abstracts, Vol. 26, No. 3-4, pp. 211-219, July 1989.

Fehler, M.C., 1989, July. Stress control of seismicity patterns observed during hydraulic fracturing experiments at the Fenton Hill hot dry rock geothermal energy site, New Mexico. In International Journal of Rock Mechanics and Mining Sciences & Geomechanics Abstracts (Vol. 26, No. 3-4, pp. 211-219). Pergamon. <https://doi.org/10.1016/0148-9062(89)91971-2>

Feng, Q., and Lees, J. M., 1998. Microseismicity, stress, and fracture in the Coso geothermal field, California. Tectonophysics, 289(1-3), pp.221-238. <https://doi.org/10.1016/S0040-1951(97)00317-X>

Feng, X.T. ed., 2017. Rock mechanics and engineering volume 2: Laboratory and field testing. CRC Press.

Flóvenz, Ó.G., Ágústsson, K., Guðnason, E.Á. and Kristjánsdóttir, S., 2015, April. Reinjection and induced seismicity in geothermal fields in Iceland. In Proceedings world geothermal congress (pp. 1-15).

Fox, A.D. and Soltanzadeh, M., 2015. A regional geomechanical study of the Duvernay Formation in Alberta, Canada. GeoConvention 2015: New Horizon, pp.4-8.

Fox, A.D. and Watson, N.D., 2019. Induced seismicity study in the Kiskatinaw seismic monitoring and mitigation area. British Columbia, report to the BC Oil and Gas Commission: Calgary, Alberta, Canada, Enlighten Geoscience.

Foxall, B., Bachmann, C. and White, J., 2017. Empirical Analysis of Seismicity Induced by Brine Injection in the US Bureau of Reclamation Paradox Valley PVU# 1 Well and Development of an Induced Earthquake Simulation Model (No. 41dcdab7-e2d5-47b0-b8ba-9141d1240a5c). National Energy Technology Laboratory (NETL), Pittsburgh, PA, Morgantown, WV, and Albany, OR (United States). Energy Data eXchange; National Energy Technology Laboratory (NETL), Pittsburgh, PA, Morgantown, WV (United States). <https://doi.org/10.18141/1433145>

Frohlich, C., DeShon, H., Stump, B., Hayward, C., Hornbach, M. and Walter, J.I., 2016. A historical review of induced earthquakes in Texas. Seismological Research Letters, 87(4), pp.1022-1038. <https://doi.org/10.1785/0220160016>

Frohlich, C., Ellsworth, W., Brown, W.A., Brunt, M., Luetgert, J., MacDonald, T. and Walter, S., 2014. The 17 May 2012 M4. 8 earthquake near Timpson, East Texas: An event possibly triggered by fluid injection. Journal of Geophysical Research: Solid Earth, 119(1), pp.581-593. <https://doi.org/10.1002/2013JB010755>

Frohlich, C., Hayward, C., Stump, B. and Potter, E., 2011. The Dallas–Fort Worth earthquake sequence: October 2008 through May 2009. Bulletin of the Seismological Society of America, 101(1), pp.327-340. <https://doi.org/10.1785/0120100131>

Frohlich, C., Potter, E., Hayward, C. and Stump, B., 2010. Dallas-Fort Worth earthquakes coincident with activity associated with natural gas production. The Leading Edge, 29(3), pp.270-275. <https://doi.org/10.1190/1.3353720>

Fulignati, P., Marianelli, P., Sbrana, A. and Ciani, V., 2014. 3D geothermal modelling of the Mount Amiata hydrothermal system in Italy. Energies, 7(11), pp.7434-7453. <https://doi.org/10.3390/en7117434>

Gaite, B., Ugalde, A., Villaseñor, A. and Blanch, E., 2016. Improving the location of induced earthquakes associated with an underground gas storage in the Gulf of Valencia (Spain). Physics of the Earth and Planetary Interiors, 254, pp.46-59. <https://doi.org/10.1016/j.pepi.2016.03.006>

Galloway, E., Hauck, T., Corlett, H., Panǎ, D., Schultz, R., 2018. Faults and associated karst collapse suggest conduits for fluid flow that influence hydraulic fracturinginduced seismicity. Proceedings of the National Academy of Sciences of the United States of America 115, E10003--E10012. <https://doi.org/10.1073/pnas.1807549115>

Gan, Q., Feng, Z., Zhou, L., Li, H., Liu, J., and Elsworth, D., 2021. Down-dip circulation at the united downs deep geothermal power project maximizes heat recovery and minimizes seismicity. Geothermics, 96, pp.102204. <https://doi.org/10.1016/j.geothermics.2021.102204>

García-Sánchez, L., Macías, J.L., Sosa-Ceballos, G., Arce, J.L., Garduño-Monroy, V.H., Saucedo, R., Avellán, D.R., Rangel, E., Layer, P.W., López-Loera, H. and Rocha, V.S., 2017. Genesis and evolution of the Cerro Prieto volcanic complex, Baja California, Mexico. Bulletin of Volcanology, 79(6), pp.1-28. <https://doi.org/10.1007/s00445-017-1126-8>

Garcia, J., Hartline, C., Walters, M., Wright, M., Rutqvist, J., Dobson, P.F. and Jeanne, P., 2016. The Northwest Geysers EGS demonstration project, California: Part 1: characterization and reservoir response to injection. Geothermics, 63, pp.97-119. <https://doi.org/10.1016/j.geothermics.2015.08.003>

Gaucher, E., Schoenball, M., Heidbach, O., Zang, A., Fokker, P., van Wees, J.D. and Kohl, T., 2015, April. Induced seismicity in geothermal reservoirs: Physical processes and key parameters. In World Geothermal Congress (pp. 1-13).

Genter, A., Evans, K., Cuenot, N., Fritsch, D. and Sanjuan, B., 2010. Contribution of the exploration of deep crystalline fractured reservoir of Soultz to the knowledge of enhanced geothermal systems (EGS). Comptes Rendus Geoscience, 342(7-8), pp.502-516. <https://doi.org/10.1016/j.crte.2010.01.006>

Ghanizadeh, A., Bhowmik, S., Haeri-Ardakani, O., Sanei, H., Clarkson, C.R., 2015. A comparison of shale permeability coefficients derived using multiple non-steady-state measurement techniques: Examples from the Duvernay Formation, Alberta (Canada). Fuel 140, 371–387. <https://doi.org/10.1016/j.fuel.2014.09.073>

Gischig, V.S., Giardini, D., Amann, F., Hertrich, M., Krietsch, H., Loew, S., Maurer, H., Villiger, L., Wiemer, S., Bethmann, F. and Brixel, B., 2020. Hydraulic stimulation and fluid circulation experiments in underground laboratories: Stepping up the scale towards engineered geothermal systems. Geomechanics for Energy and the Environment, 24, p.100175. <https://doi.org/10.1016/j.gete.2019.100175>

Glowacka, E. and Nava, F.A., 1996. Major earthquakes in Mexicali Valley, Mexico, and fluid extraction at Cerro Prieto geothermal field. Bulletin of the Seismological Society of America, 86(1A), pp.93-105. <https://doi.org/10.1785/BSSA08601A0093>

Glowacka, E., Sarychikhina, O. and Nava, F.A., 2005. Subsidence and stress change in the Cerro Prieto geothermal field, BC, Mexico. pure and applied geophysics, 162(11), pp.2095-2110. <https://doi.org/10.1007/s00024-005-2706-7>

Glowacka, E., Sarychikhina, O.L.G.A., Nava, F.A., Suarez, F., Ramírez, J., Guzman, M., Robles, B., Farfan, F. and De Cossio Batani, G.D., 2010. Continuous monitoring techniques of fault displacement caused by geothermal fluid extraction in the Cerro Prieto Geothermal Field (Baja California, Mexico). Land Subsidence, Associated Hazards and the Role of Natural Resources, edited by: Correón-Freyre D., Cerca, M., and Galowey, D., IAHS Publ, 339, pp.326-332.

Goebel, T. H. W., Hauksson, E., Aminzadeh, F., and Ampuero, J. P., 2015. An objective method for the assessment of fluid injection‐induced seismicity and application to tectonically active regions in central California. Journal of Geophysical Research: Solid Earth, 120(10), pp.7013-7032. <https://doi.org/10.1002/2015JB011895>

Goebel, T. H. W., Weingarten, M., Chen, X., Haffener, J., and Brodsky, E. E., 2017. The 2016 Mw5. 1 Fairview, Oklahoma earthquakes: Evidence for long-range poroelastic triggering at > 40 km from fluid disposal wells. Earth and Planetary Science Letters, 472, pp.50-61. <https://doi.org/10.1016/j.epsl.2017.05.011>

Goebel, T. H., Hosseini, S. M., Cappa, F., Hauksson, E., Ampuero, J. P., Aminzadeh, F., and Saleeby, J. B., 2016. Wastewater disposal and earthquake swarm activity at the southern end of the Central Valley, California. Geophysical Research Letters, 43(3), pp.1092-1099. <https://doi.org/10.1002/2015GL066948>

Goebel, T.H.W., Weingarten, M., Chen, X., Haffener, J. and Brodsky, E.E., 2017. The 2016 Mw5. 1 Fairview, Oklahoma earthquakes: Evidence for long-range poroelastic triggering at> 40 km from fluid disposal wells. Earth and Planetary Science Letters, 472, pp.50-61. <https://doi.org/10.1016/j.epsl.2017.05.011>

Goertz‐Allmann, B.P., Gibbons, S.J., Oye, V., Bauer, R. and Will, R., 2017. Characterization of induced seismicity patterns derived from internal structure in event clusters. Journal of Geophysical Research: Solid Earth, 122(5), pp.3875-3894. <https://doi.org/10.1002/2016JB013731>

Goodfellow, S.D., Nasseri, M.H.B., Maxwell, S.C. and Young, R.P., 2015. Hydraulic fracture energy budget: Insights from the laboratory. Geophysical Research Letters, 42(9), pp.3179-3187. <https://doi.org/10.1002/2015GL063093>

Grigoli, F., Cesca, S., Rinaldi, A.P., Manconi, A., Lopez-Comino, J.A., Clinton, J.F., Westaway, R., Cauzzi, C., Dahm, T. and Wiemer, S., 2018. The November 2017 M w 5.5 Pohang earthquake: A possible case of induced seismicity in South Korea. Science, 360(6392), pp.1003-1006. DOI: 10.1126/science.aat2010

Groos, J., Zeiß, J., Grund, M. and Ritter, J., 2013, April. Microseismicity at two geothermal power plants at Landau and Insheim in the Upper Rhine Graben, Germany. In Geophys. Res. Abstr (Vol. 15).

Guglielmi, Y., Birkholzer, J., Rutqvist, J., Jeanne, P. and Nussbaum, C., 2017. Can fault leakage occur before or without reactivation? Results from an in situ fault reactivation experiment at Mont Terri. Energy Procedia, 114, pp.3167-3174. <https://doi.org/10.1016/j.egypro.2017.03.1445>

Guglielmi, Y., Cappa, F., Avouac, J.P., Henry, P. and Elsworth, D., 2015. Seismicity triggered by fluid injection–induced aseismic slip. Science, 348(6240), pp.1224-1226. 10.1126/science.aab0476

Guglielmi, Y., Nussbaum, C., Jeanne, P., Rutqvist, J., Cappa, F. and Birkholzer, J., 2020. Complexity of fault rupture and fluid leakage in shale: insights from a controlled fault activation experiment. Journal of Geophysical Research: Solid Earth, 125(2), p.e2019JB017781. <https://doi.org/10.1029/2019JB017781>

Guglielmi, Y., Nussbaum, C., Rutqvist, J., Cappa, F., Jeanne, P. and Birkholzer, J., 2020. Estimating perturbed stress from 3-D borehole displacements induced by fluid injection in fractured or faulted shales. Geophysical Journal International, 221(3), pp.1684-1695. <https://doi.org/10.1093/gji/ggaa103>

Guglielmi, Y.G., Henry, P., Nussbaum, C., Dick, P., Gout, C. and Amann, F., 2015, June. Underground Research Laboratories for conducting fault activation experiments in shales. In 49th US rock mechanics/geomechanics symposium. OnePetro.

Haimson, B.C. and Chang, C., 2002. True triaxial strength of the KTB amphibolite under borehole wall conditions and its use to estimate the maximum horizontal in situ stress. Journal of Geophysical Research: Solid Earth, 107(B10), pp.ETG-15. <https://doi.org/10.1029/2001JB000647>

Haimson, B.C. and Voight, B., 1977. Crustal stress in Iceland. pure and applied geophysics, 115(1), pp.153-190. https://doi.org/10.1007/BF01637102

Hakami, E., 2009. Rock mechanics Laxemar: site descriptive modelling SDM-Site Laxemar. SKB.

Häring, M.O., Schanz, U., Ladner, F. and Dyer, B.C., 2008. Characterisation of the Basel 1 enhanced geothermal system. Geothermics, 37(5), pp.469-495. <https://doi.org/10.1016/j.geothermics.2008.06.002>

Hasting, M., Albaric, J., Oye, V., Reid, P., Messeiller, M., Llanos, E., Malin, P., Shalev, E., Hogg, M., Alvarez, M. and Miller, A., 2011, November. Real-time induced seismicity monitoring during wellbore stimulation at Paralana-2 South Australia. In Proceedings of the New Zealand Geothermal Workshop 2011 (pp. 1-9).

Hasting, M., Albaric, J., Oye, V., Reid, R., Messeiller, M., Llanos, E., Malin, P., Shalev, E., Hogg, M., Alvarez, M., Miller, A., Walter, C., Boese, C., Voss, N.: Real‐time induced seismicity monitoring during wellbore stimulation at Paralana‐2, South Australia, in: Australian Geothermal Energy Conference, 2011.

He, X.L., Li, H.B., Wang, H., Zhang, L., Xu, Z.Q. and Si, J.L., 2018. Creeping along the Guanxian‐Anxian fault of the 2008 Mw 7.9 Wenchuan earthquake in the Longmen Shan, China. Tectonics, 37(7), pp.2124-2141. <https://doi.org/10.1029/2017TC004820>

Heap, M.J., Kushnir, A.R., Vasseur, J., Wadsworth, F.B., Harlé, P., Baud, P., Kennedy, B.M., Troll, V.R. and Deegan, F.M., 2020. The thermal properties of porous andesite. Journal of Volcanology and Geothermal Research, 398, p.106901. <https://doi.org/10.1016/j.jvolgeores.2020.106901>

Heap, M.J., Villeneuve, M., Albino, F., Farquharson, J.I., Brothelande, E., Amelung, F., Got, J.L. and Baud, P., 2020. Towards more realistic values of elastic moduli for volcano modelling. Journal of volcanology and geothermal research, 390, p.106684. <https://doi.org/10.1016/j.jvolgeores.2019.106684>

Hedtmann, N. and Alber, M., 2017. Investigation of Water-permeability and Ultrasonic Wave Velocities of German Malm Aquifer Rocks for Hydro-Geothermal Energy. Procedia Engineering, 191, pp.127-133. <https://doi.org/10.1016/j.proeng.2017.05.163>

Heinemann, B.B., Troschke, B. and Tenzer, H., 1992. Hydraulic investigations and stress evaluations at the HDR test site Urach III, Germany. GEOTHERMAL RESOURCES COUNCIL, DAVIS, CA(USA)., 16, pp.425-431.

Hennings, P.H., Snee, J.E.L., Osmond, J.L., DeShon, H.R., Dommisse, R., Horne, E., Lemons, C. and Zoback, M.D., 2019. Injection‐Induced Seismicity and Fault‐Slip Potential in the Fort Worth Basin, Texas. Bulletin of the Seismological Society of America, 109(5), pp.1615-1634. <https://doi.org/10.1785/0120190017>

Hickman, S.H. and Davatzes, N.C., 2010. In-situ stress and fracture characterization for planning of an EGS stimulation in the Desert Peak Geothermal Field, Nevada.

Hillers, G., T. Vuorinen, T. A., Uski, M. R., Kortström, J. T., Mäntyniemi, P. B., Tiira, T., Malin, P.E., and Saarno, T., 2020. The 2018 geothermal reservoir stimulation in Espoo/Helsinki, Southern Finland: Seismic network anatomy and data features. Seismological Research Letters, 91(2A), pp.770-786. <https://doi.org/10.1785/0220190253>

Hofmann, H., Zimmermann, G., Farkas, M., Huenges, E., Zang, A., Leonhardt, M., Kwiatek, G., Martinez-Garzon, P., Bohnhoff, M., Min, K.B. and Fokker, P., 2019. First field application of cyclic soft stimulation at the Pohang Enhanced Geothermal System site in Korea. Geophysical Journal International, 217(2), pp.926-949. <https://doi.org/10.1093/gji/ggz058>

Hofmann, H., Zimmermann, G., Huenges, E., Regenspurg, S., Aldaz, S., Milkereit, C., Heimann, S., Dahm, T., Zang, A., Grigoli, F. and Karvounis, D., 2021. Soft stimulation treatment of geothermal well RV-43 to meet the growing heat demand of Reykjavik. Geothermics, 96, p.102146. <https://doi.org/10.1016/j.geothermics.2021.102146>

Holl, H.G. and Barton, C., 2015, April. Habanero field-structure and state of stress. In Proceedings World Geothermal Congress (pp. 19-25).

Holland, A., 2011. Examination of possibly induced seismicity from hydraulic fracturing in the Eola Field, Garvin County, Oklahoma (p. 28). Oklahoma: Oklahoma Geological Survey.

Holland, A.: Examination of Possibly Induced Seismicity from Hydraulic Fracturing in the Eola Field, Garvin County, Oklahoma, Open-File, 1–31, 2011.

Holland, A.A., 2013a. Earthquakes triggered by hydraulic fracturing in south‐central Oklahoma. Bulletin of the Seismological Society of America, 103(3), pp.1784-1792. <https://doi.org/10.1785/0120120109>

Holland, A.A., 2013b. Optimal fault orientations within Oklahoma. Seismological Research Letters, 84(5), pp.876-890. <https://doi.org/10.1785/0220120153>

Hornbach, M.J., DeShon, H.R., Ellsworth, W.L., Stump, B.W., Hayward, C., Frohlich, C., Oldham, H.R., Olson, J.E., Magnani, M.B., Brokaw, C. and Luetgert, J.H., 2015. Causal factors for seismicity near Azle, Texas. Nature communications, 6(1), pp.1-11. <https://doi.org/10.1038/ncomms7728>

Hornbach, M.J., Jones, M., Scales, M., DeShon, H.R., Magnani, M.B., Frohlich, C., Stump, B., Hayward, C. and Layton, M., 2016. Ellenburger wastewater injection and seismicity in North Texas. Physics of the Earth and Planetary Interiors, 261, pp.54-68. <https://doi.org/10.1016/j.pepi.2016.06.012>

Horton, S., 2012. Disposal of hydrofracking waste fluid by injection into subsurface aquifers triggers earthquake swarm in central Arkansas with potential for damaging earthquake. Seismological Research Letters, 83(2), pp.250-260. <https://doi.org/10.1785/gssrl.83.2.250>

Hsieh, P.A. and Bredehoeft, J.D., 1981. A reservoir analysis of the Denver earthquakes: A case of induced seismicity. Journal of Geophysical Research: Solid Earth, 86(B2), pp.903-920. <https://doi.org/10.1029/JB086iB02p00903>

Huang, Y. and Beroza, G.C., 2015. Temporal variation in the magnitude‐frequency distribution during the Guy‐Greenbrier earthquake sequence. Geophysical Research Letters, 42(16), pp.6639-6646. <https://doi.org/10.1002/2015GL065170>

Huang, Y., Beroza, G.C. and Ellsworth, W.L., 2016. Stress drop estimates of potentially induced earthquakes in the Guy‐Greenbrier sequence. Journal of Geophysical Research: Solid Earth, 121(9), pp.6597-6607. <https://doi.org/10.1002/2016JB013067>

Huenges, E., Erzinger, J., Kück, J., Engeser, B. and Kessels, W., 1997. The permeable crust: Geohydraulic properties down to 9101 m depth. Journal of Geophysical Research: Solid Earth, 102(B8), pp.18255-18265. <https://doi.org/10.1029/96JB03442>

Hui, G., Chen, S. and Gu, F., 2020, September. Insights on Trigger Mechanisms of Two Large Hydraulic Fracturing-Induced Earthquakes and Sensitivity Analysis. In SPE Canada Unconventional Resources Conference. OnePetro. <https://doi.org/10.2118/199996-MS>

Hui, G., Chen, S., Chen, Z. and Gu, F., 2021. An integrated approach to characterize hydraulic fracturing-induced seismicity in shale reservoirs. Journal of Petroleum Science and Engineering, 196, p.107624. <https://doi.org/10.1016/j.petrol.2020.107624>

Hui, G., Chen, S., Chen, Z., He, Y., Wang, S. and Gu, F., 2021. Investigation on two Mw 3.6 and Mw 4.1 earthquakes triggered by poroelastic effects of hydraulic fracturing operations near crooked lake, Alberta. Journal of Geophysical Research: Solid Earth, 126(5), p.e2020JB020308. <https://doi.org/10.1029/2020JB020308>

Hui, G., Chen, S., Chen, Z., Jing, G., Hu, D. and Gu, F., 2021. Role of Fluid Diffusivity in the Spatiotemporal Migration of Induced Earthquakes during Hydraulic Fracturing in Unconventional Reservoirs. Energy & Fuels, 35(21), pp.17685-17697. <https://doi.org/10.1021/acs.energyfuels.1c02950>

Hui, G., Chen, S., Gu, F., Pang, Y., Yu, X. and Zhang, L., 2021. Insights on controlling factors of hydraulically induced seismicity in the Duvernay East Shale Basin. Geochemistry, Geophysics, Geosystems, 22(2), p.e2020GC009563. <https://doi.org/10.1029/2020GC009563>

Hulen, J.B., Kaspereit, D., Norton, D.L., Osborn, W., Pulka, F.S. and Bloomquist, R., 2002. Refined conceptual modeling and a new resource estimate for the Salton Sea geothermal field, Imperial Valley, California. TRANSACTIONS-GEOTHERMAL RESOURCES COUNCIL, pp.29-36.

Humphreys, B., Hodson-Clarke, A. and Hogarth, R., 2014. Habanero Geothermal Project Field Development Plan. Geodynamics Ltd.

Iding, M. and Ringrose, P., 2010. Evaluating the impact of fractures on the performance of the In Salah CO2 storage site. International Journal of Greenhouse Gas Control, 4(2), pp.242-248. <https://doi.org/10.1016/j.ijggc.2009.10.016>

Igonin, N., Verdon, J.P., Kendall, J.M. and Eaton, D.W., 2021. Large‐scale fracture systems are permeable pathways for fault activation during hydraulic fracturing. Journal of Geophysical Research: Solid Earth, 126(3), p.e2020JB020311. <https://doi.org/10.1029/2020JB020311>

Igonin, N., Zecevic, M., Eaton, D.W., 2018. Bilinear Magnitude-Frequency Distributions and Characteristic Earthquakes During Hydraulic Fracturing. Geophysical Research Letters 45, 12,812-866,874. <https://doi.org/10.1029/2018GL079746>

Improta, L., Bagh, S., De Gori, P., Valoroso, L., Pastori, M., Piccinini, D., Chiarabba, C., Anselmi, M. and Buttinelli, M., 2017. Reservoir structure and wastewater‐induced seismicity at the Val d'Agri Oilfield (Italy) shown by three‐dimensional Vp and Vp/Vs local earthquake tomography. Journal of Geophysical Research: Solid Earth, 122(11), pp.9050-9082. <https://doi.org/10.1002/2017JB014725>

Improta, L., Valoroso, L., Piccinini, D. and Chiarabba, C., 2015. A detailed analysis of wastewater‐induced seismicity in the Val d'Agri oil field (Italy). Geophysical Research Letters, 42(8), pp.2682-2690. <https://doi.org/10.1002/2015GL063369>

Jacquey, A. B., Cacace, M., Blöcher, G., Watanabe, N., Huenges, E., and Scheck-Wenderoth, M., 2016. Thermo-poroelastic numerical modelling for enhanced geothermal system performance: Case study of the Groß Schönebeck reservoir. Tectonophysics, 684, pp.119-130. <https://doi.org/10.1016/j.tecto.2015.12.020>

Jeanne, P., Guglielmi, Y. and Cappa, F., 2012. Multiscale seismic signature of a small fault zone in a carbonate reservoir: Relationships between VP imaging, fault zone architecture and cohesion. Tectonophysics, 554, pp.185-201. <https://doi.org/10.1016/j.tecto.2012.05.012>

Jeanne, P., Guglielmi, Y., Lamarche, J., Cappa, F. and Marié, L., 2012. Architectural characteristics and petrophysical properties evolution of a strike-slip fault zone in a fractured porous carbonate reservoir. Journal of Structural Geology, 44, pp.93-109. <https://doi.org/10.1016/j.jsg.2012.08.016>

Jeanne, P., Guglielmi, Y., Rutqvist, J., Nussbaum, C. and Birkholzer, J., 2017. Field characterization of elastic properties across a fault zone reactivated by fluid injection. Journal of Geophysical Research: Solid Earth, 122(8), pp.6583-6598. <https://doi.org/10.1002/2017JB014384>

Ji, Y., Yoon, J.S., Zang, A. and Wu, W., 2021. Mitigation of injection-induced seismicity on undrained faults in granite using cyclic fluid injection: A laboratory study. International Journal of Rock Mechanics and Mining Sciences, 146, p.104881. <https://doi.org/10.1016/j.ijrmms.2021.104881>

Jing, Y., Jing, Z., Willis-Richards, J., and Hashida, T., 2014. A simple 3-D thermoelastic model for assessment of the long-term performance of the Hijiori deep geothermal reservoir. Journal of volcanology and geothermal research, 269, pp.14-22. <https://doi.org/10.1016/j.jvolgeores.2013.10.012>

Jing, Z., Willis‐Richards, J., Watanabe, K. and Hashida, T., 2000. A three‐dimensional stochastic rock mechanics model of engineered geothermal systems in fractured crystalline rock. Journal of Geophysical Research: Solid Earth, 105(B10), pp.23663-23679. <https://doi.org/10.1029/2000JB900202>

Johann, L., and Shapiro, S. A., 2020. Understanding Vectorial Migration Patterns of Wastewater‐Induced Earthquakes in the United States. Bulletin of the Seismological Society of America, 110(5), pp.2295-2307. <https://doi.org/10.1785/0120200064>

Juanes, R., Castiñeira, D., Fehler, M.C., Hager, B.H., Jha, B., Shaw, J.H. and Plesch, A., 2017. Coupled flow and geomechanical modeling, and assessment of induced seismicity, at the Castor underground gas storage project. Final Report, pp.1-86.

Julian, B. R., Foulger, G. R., and Monastero, F. C.: Seismic monitoring of EGS stimulation tests at the Coso geothermal field, California, using microearthquake locations and moment tensors, in: Thirty-Fourth Workshop on Geothermal Reservoir Engineering, Stanford University, Stanford, California, 9-11, February 2009.

Juncu, D., Árnadóttir, T., Geirsson, H., Guðmundsson, G.B., Lund, B., Gunnarsson, G., Hooper, A., Hreinsdottir, S. and Michalczewska, K., 2020. Injection-induced surface deformation and seismicity at the Hellisheidi geothermal field, Iceland. Journal of Volcanology and Geothermal Research, 391, p.106337. <https://doi.org/10.1016/j.jvolgeores.2018.03.019>

Juncu, D., Árnadóttir, T., Hooper, A. and Gunnarsson, G., 2017. Anthropogenic and natural ground deformation in the Hengill geothermal area, Iceland. Journal of Geophysical Research: Solid Earth, 122(1), pp.692-709. <https://doi.org/10.1002/2016JB013626>

Jupe, A. J., Green, A. S. P., and Wallroth, T.w: Induced microseismicity and reservoir growth at the Fjällbacka hot dry rocks project, Sweden, in: International journal of rock mechanics and mining sciences and geomechanics abstracts (Vol. 29, No. 4, pp. 343-354), July 1992. <https://doi.org/10.1016/0148-9062(92)90511-W>

Justinic, A.H., Stump, B., Hayward, C. and Frohlich, C., 2013. Analysis of the Cleburne, Texas, earthquake sequence from June 2009 to June 2010. Bulletin of the Seismological Society of America, 103(6), pp.3083-3093. <https://doi.org/10.1785/0120120336>

Kaieda, H., Ito, H., Kiho, K., Suzuki, K., Suenaga, H. and Shin, K., 2005, April. Review of the Ogachi HDR project in Japan. In Proceedings of the world geothermal congress.

Kaieda, H., Jones, R., Moriya, H., Sasaki, S. and Ushijima, K., 2000, April. Ogachi HDR reservoir evaluation by AE and geophysical methods. In Proceedings of world geothermal congress (pp. 24-29).

Kaieda, H., Sasaki, S. and Wyborn, D., 2010, April. Comparison of characteristics of micro-earthquakes observed during hydraulic stimulation operations in Ogachi, Hijiori and Cooper Basin HDR projects. In Proceedings of the World Geothermal Congress.

Kaieda, H., Sasaki, S., and Wyborn, D.: Comparison of characteristics of micro-earthquakes observed during hydraulic stimulation operations in Ogachi, Hijiori and Cooper Basin HDR projects, in: Proceedings of the World Geothermal Congress, April 2010.

Kakurina, M., Guglielmi, Y., Nussbaum, C. and Valley, B., 2020. In situ direct displacement information on fault reactivation during fluid injection. Rock Mechanics and Rock Engineering, 53(10), pp.4313-4328. <https://doi.org/10.1007/s00603-020-02160-w>

Kaspereit, D., Mann, M., Sanyal, S., Rickard, B., Osborn, W. and Hulen, J., 2016. Updated conceptual model and reserve estimate for the Salton Sea geothermal field, Imperial Valley, California. Geotherm. Res. Council Trans, 40, pp.57-66.

Keiding, M., Árnadóttir, T., Jónsson, S., Decriem, J. and Hooper, A., 2010. Plate boundary deformation and man-made subsidence around geothermal fields on the Reykjanes Peninsula, Iceland. Journal of Volcanology and Geothermal Research, 194(4), pp.139-149. <https://doi.org/10.1016/j.jvolgeores.2010.04.011>

Keilegavlen, E., Duboeuf, L., Dichiarante, A.M., Halldórsdóttir, S., Stefansson, I., Naumann, M., Guðnason, E.Á., Ágústsson, K., Eggertsson, G.H., Oye, V. and Berre, I., 2021. Hydro-mechanical simulation and analysis of induced seismicity for a hydraulic stimulation test at the Reykjanes geothermal field, Iceland. Geothermics, 97, p.102223. <https://doi.org/10.1016/j.geothermics.2021.102223>

Keranen, K. M., Savage, H. M., Abers, G. A., and Cochran, E. S., 2013. Potentially induced earthquakes in Oklahoma, USA: Links between wastewater injection and the 2011 Mw 5.7 earthquake sequence. Geology, 41(6), pp.699-702. <https://doi.org/10.1130/G34045.1>

Keranen, K.M., Weingarten, M., Abers, G.A., Bekins, B.A. and Ge, S., 2014. Sharp increase in central Oklahoma seismicity since 2008 induced by massive wastewater injection. Science, 345(6195), pp.448-451. DOI: 10.1126/science.1255802

Keranen, K.M., Weingarten, M., Abers, G.A., Bekins, B.A. and Ge, S., 2014. Sharp increase in central Oklahoma seismicity since 2008 induced by massive wastewater injection. Science, 345(6195), pp.448-451. <https://www.science.org/doi/abs/10.1126/science.1255802>

Kettlety, T. and Verdon, J.P., 2021. Fault triggering mechanisms for hydraulic fracturing-induced seismicity from the Preston New Road, UK Case Study. Frontiers in Earth Science, 9, p.670771. <https://doi.org/10.3389/feart.2021.670771>

Kettlety, T., Verdon, J.P., Butcher, A., Hampson, M. and Craddock, L., 2021. High‐resolution imaging of the ML 2.9 August 2019 earthquake in Lancashire, United Kingdom, induced by hydraulic fracturing during Preston New Road PNR‐2 operations. Seismological Research Letters, 92(1), pp.151-169. <https://doi.org/10.1785/0220200187>

Kettlety, T., Verdon, J.P., Werner, M.J., Kendall, J.M. and Budge, J., 2019. Investigating the role of elastostatic stress transfer during hydraulic fracturing-induced fault activation. Geophysical Journal International, 217(2), pp.1200-1216. <https://doi.org/10.1093/gji/ggz080>

Kilic, D. and Tapp, B., 2013. Structural analysis of the Eola-Robberson Field using balanced cross sections, Garvin County, Oklahoma (Doctoral dissertation, University of Tulsa).

Kim, H., Xie, L., Min, K.B., Bae, S. and Stephansson, O., 2017. Integrated in situ stress estimation by hydraulic fracturing, borehole observations and numerical analysis at the EXP-1 borehole in Pohang, Korea. Rock Mechanics and Rock Engineering, 50(12), pp.3141-3155. <https://doi.org/10.1007/s00603-017-1284-1>

Kim, K.H., Ree, J.H., Kim, Y., Kim, S., Kang, S.Y. and Seo, W., 2018. Assessing whether the 2017 M w 5.4 Pohang earthquake in South Korea was an induced event. Science, 360(6392), pp.1007-1009. 10.1126/science.aat6081

Kim, K.I., Min, K.B., Kim, K.Y., Choi, J.W., Yoon, K.S., Yoon, W.S., Yoon, B., Lee, T.J. and Song, Y., 2018. Protocol for induced microseismicity in the first enhanced geothermal systems project in Pohang, Korea. Renewable and Sustainable Energy Reviews, 91, pp.1182-1191. <https://doi.org/10.1016/j.rser.2018.04.062>

Kim, W.Y., 2013. Induced seismicity associated with fluid injection into a deep well in Youngstown, Ohio. Journal of Geophysical Research: Solid Earth, 118(7), pp.3506-3518. <https://doi.org/10.1002/jgrb.50247>

Kirichek, A., 2018. Electrokinetic and poroelastic Characterization of Porous Media: Application to CO2 Storage Monitoring (Doctoral dissertation, Delft University of Technology).

Kraft, T. and Deichmann, N., 2014. High-precision relocation and focal mechanism of the injection-induced seismicity at the Basel EGS. Geothermics, 52, pp.59-73. <http://dx.doi.org/10.1016/j.geothermics.2014.05.014>

Krietsch, H., Gischig, V., Evans, K., Doetsch, J., Dutler, N.O., Valley, B. and Amann, F., 2019. Stress measurements for an in situ stimulation experiment in crystalline rock: integration of induced seismicity, stress relief and hydraulic methods. Rock Mechanics and Rock Engineering, 52(2), pp.517-542. <https://doi.org/10.1007/s00603-018-1597-8>

Krietsch, H., Gischig, V.S., Doetsch, J., Evans, K.F., Villiger, L., Jalali, M., Valley, B., Löw, S. and Amann, F., 2020. Hydromechanical processes and their influence on the stimulation effected volume: observations from a decameter-scale hydraulic stimulation project. Solid Earth, 11(5), pp.1699-1729. <https://doi.org/10.5194/se-11-1699-2020>

Kroll, K.A., Cochran, E.S. and Murray, K.E., 2017. Poroelastic properties of the Arbuckle Group in Oklahoma derived from well fluid level response to the 3 September 2016 M w 5.8 Pawnee and 7 November 2016 M w 5.0 Cushing earthquakes. Seismological Research Letters, 88(4), pp.963-970. <https://doi.org/10.1785/0220160228>

Kruszewski, M., Montegrossi, G., Montes, M.R., Wittig, V., Garcia, A.G., Luviano, M.S. and Bracke, R., 2019. A wellbore cement sheath damage prediction model with the integration of acoustic wellbore measurements. Geothermics, 80, pp.195-207. <https://doi.org/10.1016/j.geothermics.2019.03.007>

Küperkoch, L., Olbert, K. and Meier, T., 2018. Long‐term monitoring of induced seismicity at the Insheim geothermal site, Germany. Bulletin of the Seismological Society of America, 108(6), pp.3668-3683. <https://doi.org/10.1785/0120170365>

Kushnir, A.R., Heap, M.J., Baud, P., Gilg, H.A., Reuschlé, T., Lerouge, C., Dezayes, C. and Duringer, P., 2018. Characterizing the physical properties of rocks from the Paleozoic to Permo-Triassic transition in the Upper Rhine Graben. Geothermal Energy, 6(1), pp.1-32. <https://doi.org/10.1186/s40517-018-0103-6>

Kwiatek, G., Bulut, F., Bohnhoff, M. and Dresen, G., 2014. High-resolution analysis of seismicity induced at Berlín geothermal field, El Salvador. Geothermics, 52, pp.98-111. <https://doi.org/10.1016/j.geothermics.2013.09.008>

Kwiatek, G., Martínez‐Garzón, P., Plenkers, K., Leonhardt, M., Zang, A., Von Specht, S., Dresen, G. and Bohnhoff, M., 2018. Insights into complex subdecimeter fracturing processes occurring during a water injection experiment at depth in Äspö Hard Rock Laboratory, Sweden. Journal of Geophysical Research: Solid Earth, 123(8), pp.6616-6635. <https://doi.org/10.1029/2017JB014715>

Kwiatek, G., Saarno, T., Ader, T., Bluemle, F., Bohnhoff, M., Chendorain, M., Dresen, G., Heikkinen, P., Kukkonen I., Leary, P., Leonhardt, M., Malin, P., Martínez-Garzón, P., Passmore, K., Passmore, P., Valenzuela, S., and Wollin, C., 2019. Controlling fluid-induced seismicity during a 6.1-km-deep geothermal stimulation in Finland. Science Advances, 5(5), eaav7224. <https://doi.org/10.1126/sciadv.aav7224>

Kwiatek, G., Saarno, T., Ader, T., Bluemle, F., Bohnhoff, M., Chendorain, M., Dresen, G., Heikkinen, P., Kukkonen, I., Leary, P. and Leonhardt, M., 2019. Controlling fluid-induced seismicity during a 6.1-km-deep geothermal stimulation in Finland. Science Advances, 5(5), p.eaav7224. 10.1126/sciadv.aav7224

Kwon, S., Xie, L., Park, S., Kim, K.I., Min, K.B., Kim, K.Y., Zhuang, L., Choi, J., Kim, H. and Lee, T.J., 2019. Characterization of 4.2-km-deep fractured granodiorite cores from Pohang Geothermal Reservoir, Korea. Rock Mechanics and Rock Engineering, 52(3), pp.771-782. <https://doi.org/10.1007/s00603-018-1639-2>

Laenen, B., Schöffer, S. I., Baisch, Q. C. S., Slob, C. C. S., and Laenen, V. B., 2020. Project KEM-06. <https://doi.org/10.5911/20-006.071>

Lashin, A., 2005. Reservoir parameter estimation using well logging data and production history of the Kaldárholt geothermal field, S-Iceland. United Nations University.

Ledingham, P., Cotton, L., and Law, R.: The united downs deep geothermal power project, in: Proceedings of the 44th Workshop on Geothermal Reservoir Engineering, Stanford University, Stanford, CA, USA (pp. 11-13), February 2019.

Lei, X., Huang, D., Su, J., Jiang, G., Wang, X., Wang, H., Guo, X. and Fu, H., 2017. Fault reactivation and earthquakes with magnitudes of up to Mw4. 7 induced by shale-gas hydraulic fracturing in Sichuan Basin, China. Scientific reports, 7(1), pp.1-12. <https://doi.org/10.1038/s41598-017-08557-y>

Lei, X., Wang, Z. and Su, J., 2019. Possible link between long‐term and short‐term water injections and earthquakes in salt mine and shale gas site in Changning, south Sichuan Basin, China. Earth and Planetary Physics, 3(6), pp.510-525. <https://doi.org/10.26464/epp2019052>

Lei, X., Wang, Z. and Su, J., 2019. The December 2018 ML 5.7 and January 2019 ML 5.3 earthquakes in South Sichuan basin induced by shale gas hydraulic fracturing. Seismological Research Letters, 90(3), pp.1099-1110. <https://doi.org/10.1785/0220190029>

Lei, X., Wang, Z., Su, J., 2019b. Possible link between long-term and short-term water injections and earthquakes in salt mine and shale gas site in Changning, south Sichuan Basin, China. 510–525. <https://doi.org/10.26464/epp2019052>

Lei, X., Yu, G., Ma, S., Wen, X. and Wang, Q., 2008. Earthquakes induced by water injection at∼ 3 km depth within the Rongchang gas field, Chongqing, China. Journal of Geophysical Research: Solid Earth, 113(B10). <https://doi.org/10.1029/2008JB005604>

Leonhardt, M., Kwiatek, G., Martínez-Garzón, P., Bohnhoff, M., Saarno, T., Heikkinen, P. and Dresen, G., 2021. Seismicity during and after stimulation of a 6.1 km deep enhanced geothermal system in Helsinki, Finland. Solid Earth, 12(3), pp.581-594. <https://doi.org/10.5194/se-12-581-2021>

Li X.Y., LEI, X.L., LI, Q. and CUI, Y.X., 2015. Characteristics of acoustic emission during deformation and failure of typical reservoir rocks under triaxial compression: An example of Sinian dolomite and shale in the Sichuan Basin. Chinese Journal of Geophysics, 58(3), pp.982-992. <https://doi.org/10.1007/s00531-015-1285-9>

Li, H., Wang, H., Yang, G., Xu, Z., Li, T., Si, J., Sun, Z., Huang, Y., Chevalier, M.L., Zhang, W. and Zhang, J., 2016. Lithological and structural characterization of the Longmen Shan fault belt from the 3rd hole of the Wenchuan Earthquake Fault Scientific Drilling project (WFSD-3). International Journal of Earth Sciences, 105(8), pp.2253-2272. <https://doi.org/10.1007/s00531-015-1285-9>

Li, X., Lei, X., Li, Q., & Li, X. (2017). Experimental investigation of Sinian shale rock under triaxial stress monitored by ultrasonic transmission and acoustic emission. Journal of Natural Gas Science and Engineering, 43, 110–123. <https://doi.org/10.1016/j.jngse.2017.03.035>

Li, X.Y., Lei, X.L., Li, Q., Cui, Y.X., 2015. Characteristics of acoustic emission during deformation and failure of typical reservoir rocks under triaxial compression: An example of Sinian dolomite and shale in the Sichuan Basin. Acta Geophysica Sinica 58, 982–992. <https://doi.org/10.6038/cjg20150323>

Li, Y., Wang, J., Jung, W. and Ghassemi, A., 2012, January. Mechanical properties of intact rock and fractures in welded tuff from Newberry Volcano. In Proceedings of 37th Workshop on Geothermal Reservoir Engineering, Stanford, CA (Vol. 30).

Li, Z., Elsworth, D. and Wang, C., 2021. Constraining maximum event magnitude during injection-triggered seismicity. Nature communications, 12(1), pp.1-9. <https://doi.org/10.1038/s41467-020-20700-4>

Liang, C., Jiang, Z., Zhang, C., Guo, L., Yang, Y. and Li, J., 2014. The shale characteristics and shale gas exploration prospects of the Lower Silurian Longmaxi shale, Sichuan Basin, South China. Journal of Natural Gas Science and Engineering, 21, pp.636-648. <https://doi.org/10.1016/j.jngse.2014.09.034>

Lopez-Comino, J.A., Cesca, S., Jarosławski, J., Montcoudiol, N., Heimann, S., Dahm, T., Lasocki, S., Gunning, A., Capuano, P. and Ellsworth, W.L., 2018. Induced seismicity response of hydraulic fracturing: Results of a multidisciplinary monitoring at the Wysin site, Poland. Scientific reports, 8(1), pp.1-14. <https://doi.org/10.1038/s41598-018-26970-9>

Lucas, Y., Ngo, V.V., Clément, A., Fritz, B. and Schäfer, G., 2020. Modelling acid stimulation in the enhanced geothermal system of Soultz-sous-Forêts (Alsace, France). Geothermics, 85, p.101772. <https://doi.org/10.1016/j.geothermics.2019.101772>

Luke, S., 2019. Reservoir Characterization of the Point Pleasant Formation, Appalachian Basin, SE Ohio. Colorado School of Mines.

Lutz, S.J., Hickman, S., Davatzes, N., Zemach, E., Drakos, P. and Robertson-Tait, A., 2010. Rock mechanical testing in support of well stimulation activities at the desert Peak geothermal field, Nevada. Geothermal Resources Council Transactions, 34.

Ma, X., Hertrich, M., Amann, F., Bröker, K., Gholizadeh Doonechaly, N., Gischig, V., Hochreutener, R., Kästli, P., Krietsch, H., Marti, M. and Nägeli, B., 2021. Multi-disciplinary characterizations of the Bedretto Lab–a unique underground geoscience research facility. Solid Earth Discussions. <https://doi.org/10.3929/ethz-b-000510360>

Ma, X., Li, Z., Hua, P., Jiang, J., Zhao, F., Han, C., Yuan, P., Lu, S. and Peng, L., 2015. Fluidinjection-induced seismicity experiment of the WFSD-3P borehole. Acta Geol. Sin.(English Edition), 89, pp.1057-1058. <https://doi.org/10.1111/1755-6724.12506>

Maghsoudi, S., Eaton, D.W., Davidsen, J., 2016. Nontrivial clustering of microseismicity induced by hydraulic fracturing. Geophysical Research Letters 43, 10, 610-672, 679. <https://doi.org/10.1002/2016GL070983>

Mahani, A.B., Schultz, R., Kao, H., Walker, D., Johnson, J. and Salas, C., 2017. Fluid injection and seismic activity in the northern Montney play, British Columbia, Canada, with special reference to the 17 August 2015 M w 4.6 induced earthquake. Bulletin of the Seismological Society of America, 107(2), pp.542-552. <https://doi.org/10.1785/0120160175>

Majer, E.L., Baria, R., Stark, M., Oates, S., Bommer, J., Smith, B. and Asanuma, H., 2007. Induced seismicity associated with enhanced geothermal systems. Geothermics, 36(3), pp.185-222. <https://doi.org/10.1016/j.geothermics.2007.03.003>

Manga, M., Wang, C. Y., and Shirzaei, M., 2016. Increased stream discharge after the 3 September 2016 Mw 5.8 Pawnee, Oklahoma earthquake. Geophysical Research Letters, 43(22), pp.11-588. <https://doi.org/10.1002/2016GL071268>

Martinez-Baez, L.F., 1980. Thermal conductivity of core samples from the Cerro Prieto geothermal field: Experimental results and an improved prediction method. Geothermics;(United States), 9(CONF-7809252).

Martínez‐Garzón, P., Kwiatek, G., Sone, H., Bohnhoff, M., Dresen, G. and Hartline, C., 2014. Spatiotemporal changes, faulting regimes, and source parameters of induced seismicity: A case study from The Geysers geothermal field. Journal of Geophysical Research: Solid Earth, 119(11), pp.8378-8396. <https://doi.org/10.1002/2014JB011385>

Masri, M., Sibai, M., Shao, J.F. and Mainguy, M., 2014. Experimental investigation of the effect of temperature on the mechanical behavior of Tournemire shale. International Journal of Rock Mechanics and Mining Sciences, 70, pp.185-191. <https://doi.org/10.1016/j.ijrmms.2014.05.007>

Maurer, V., Gaucher, E., Grunberg, M., Koepke, R., Pestourie, R. and Cuenot, N., 2020. Seismicity induced during the development of the Rittershoffen geothermal field, France. Geothermal Energy, 8(1), pp.1-31. <https://doi.org/10.1186/s40517-020-0155-2>

Maxwell, S.C., Pope, T., Cipolla, C., Mack, M., Trimbitasu, L., Norton, M., Leonard, J., 2011. Understanding Hydraulic Fracture Variability Through Integrating Microseismicity and Seismic Reservoir Characterization, in: SPE North American Unconventional Gas Conference and Exhibition Held in The Woodlands, Texas, USA. <https://signdoi.org/10.2118/144207-MS>

Mazzoldi, A., Borgia, A., Ripepe, M., Marchetti, E., Ulivieri, G., della Schiava, M. and Allocca, C., 2015. Faults strengthening and seismicity induced by geothermal exploitation on a spreading volcano, Mt. Amiata, Italia. Journal of Volcanology and Geothermal Research, 301, pp.159-168. <https://doi.org/10.1016/j.jvolgeores.2015.05.015>

McClure, M.W. and Horne, R.N., 2014. Correlations between formation properties and induced seismicity during high pressure injection into granitic rock. Engineering geology, 175, pp.74-80. <https://doi.org/10.1016/j.enggeo.2014.03.015>

McDermott, C.I., Randriamanjatosoa, A.L., Tenzer, H., Sauter, M. and Kolditz, O., 2005, April. Pressure dependent hydraulic flow, heat transport and geo-thermo-mechanical deformation in HDR crystalline geothermal systems: preliminary application to identify energy recovery schemes at Urach Spa. In Proceedings World Geothermal Congress.

McGarr, A. and Barbour, A.J., 2017. Wastewater disposal and the earthquake sequences during 2016 near Fairview, Pawnee, and Cushing, Oklahoma. Geophysical Research Letters, 44(18), pp.9330-9336. <https://doi.org/10.1002/2017GL075258>

McGarr, A., 2014. Maximum magnitude earthquakes induced by fluid injection. Journal of Geophysical Research: solid earth, 119(2), pp.1008-1019. <https://doi.org/10.1002/2013JB010597>

McGuire, J.J., Lohman, R.B., Catchings, R.D., Rymer, M.J. and Goldman, M.R., 2015. Relationships among seismic velocity, metamorphism, and seismic and aseismic fault slip in the Salton Sea Geothermal Field region. Journal of Geophysical Research: Solid Earth, 120(4), pp.2600-2615. <https://doi.org/10.1002/2014JB011579>

McLellan, P., 2012, May. Direct shear measurements of bedding plane strength and stiffness, Montney and Doig formations, Farrell Creek field, northeast British Columbia. In Canadian Rock Mechanics Association Conference, Edmonton, Alberta.

McMahon, N.D., Aster, R.C., Yeck, W.L., McNamara, D.E. and Benz, H.M., 2017. Spatiotemporal evolution of the 2011 Prague, Oklahoma, aftershock sequence revealed using subspace detection and relocation. Geophysical Research Letters, 44(14), pp.7149-7158. <https://doi.org/10.1002/2017GL072944>

McNamara, D. E., Hayes, G. P., Benz, H. M., Williams, R. A., McMahon, N. D., Aster, R. C., Holland, A., Sickbert, T., Herrmann, R., Briggs, R., Smoczyk, G., Bergman, E., and Earle, P. (2015). Reactivated faulting near Cushing, Oklahoma: Increased potential for a triggered earthquake in an area of United States strategic infrastructure. Geophysical Research Letters, 42(20), 8328-8332. <https://doi.org/10.1002/2015GL064669>

McNamara, D.D., Massiot, C., Lewis, B. and Wallis, I.C., 2015. Heterogeneity of structure and stress in the Rotokawa Geothermal Field, New Zealand. Journal of Geophysical Research: Solid Earth, 120(2), pp.1243-1262. <https://doi.org/10.1002/2014JB011480>

Megies, T. and Wassermann, J., 2014. Microseismicity observed at a non-pressure-stimulated geothermal power plant. Geothermics, 52, pp.36-49. <https://doi.org/10.1016/j.geothermics.2014.01.002>

Melin, H., 2012. Controlling parameters for normal and shear behaviour of rock fractures-a study of direct shear test data from SKB.

Meller, C. and Ledésert, B., 2017. Is there a link between mineralogy, petrophysics, and the hydraulic and seismic behaviors of the Soultz‐sous‐Forêts granite during stimulation? A review and reinterpretation of petro‐hydromechanical data toward a Better Understanding of Induced Seismicity and Fluid Flow. Journal of Geophysical Research: Solid Earth, 122(12), pp.9755-9774. <https://doi.org/10.1002/2017JB014648>

Meller, C., 2014. Localization and characterization of hydrothermal alteration zones in a geothermal reservoir and their significance for rock mechanics. 10.5445/IR/1000044749

Mercerat, D., Souley, M., Driad-Lebeau, L. and Bernard, P., 2005, November. Induced seismicity in a salt mine environment evaluated by a coupled continuum-discrete modelling. In Symposium Post mining 2005 (p. NC).

Mignan, A., 2021. Induced Seismicity Completeness Analysis for Improved Data Mining. Frontiers in Earth Science, 9, 115p. <https://doi.org/10.3389/feart.2021.635193>

Minissale, A., 1991. The Larderello geothermal field: a review. Earth-Science Reviews, 31(2), pp.133-151. <https://doi.org/10.1016/0012-8252(91)90018-B>

Moeck, I., Bloch, T., Graf, R., Heuberger, S., Kuhn, P., Naef, H., Sonderegger, M., Uhlig, S. and Wolfgramm, M., 2015, April. The St. Gallen project: development of fault controlled geothermal systems in urban areas. In Proceedings world geothermal congress (p. 5).

Moeck, I., Kwiatek, G., and Zimmermann, G., 2009. Slip tendency analysis, fault reactivation potential and induced seismicity in a deep geothermal reservoir. Journal of Structural Geology, 31(10), pp.1174-1182. <https://doi.org/10.1016/j.jsg.2009.06.012>

Moeck, I.S., 2014. Catalog of geothermal play types based on geologic controls. Renewable and Sustainable Energy Reviews, 37, pp.867-882. <https://doi.org/10.1016/j.rser.2014.05.032>

Monterrosa, M., 2012, October. Sustainability analysis of the Berlin geothermal field, El Salvador. In Proceedings of the SIMS (pp. 4-6).

Monterrosa, M.E. and SA, G.S., 2002, January. Reservoir modelling for the Berlin geothermal field El Salvador. In Proceedings.

Morgan, B.C. and Murray, K.E., 2015. Characterizing small-scale permeability of the Arbuckle Group, Oklahoma. Okla. Geol. Surv. Open-File Rept. OF2-2015, pp.1-12.

Morgan, B.C. and Murray, K.E.: Characterizing small-scale permeability of the Arbuckle Group, Oklahoma. Okla. Geol. Surv. Open-File Rept. OF2-2015, 12 pp., 2015. <http://ogs.ou.edu/docs/openfile/OF2-2015.pdf>

Morris, J.P., Hao, Y., Foxall, W. and McNab, W., 2011. A study of injection-induced mechanical deformation at the In Salah CO2 storage project. International Journal of Greenhouse Gas Control, 5(2), pp.270-280. <https://doi.org/10.1016/j.ijggc.2010.10.004>

Mousavi, S.M., Ogwari, P.O., Horton, S.P. and Langston, C.A., 2017. Spatio-temporal evolution of frequency-magnitude distribution and seismogenic index during initiation of induced seismicity at Guy-Greenbrier, Arkansas. Physics of the Earth and Planetary Interiors, 267, pp.53-66. <https://doi.org/10.1016/j.pepi.2017.04.005>

Nakai, J.S., Weingarten, M., Sheehan, A.F., Bilek, S.L. and Ge, S., 2017. A possible causative mechanism of Raton Basin, New Mexico and Colorado earthquakes using recent seismicity patterns and pore pressure modeling. Journal of Geophysical Research: Solid Earth, 122(10), pp.8051-8065. <https://doi.org/10.1002/2017JB014415>

Neuhaus, C.W., Miskimins, J.L., 2012. Analysis of Surface and Downhole Microseismic Monitoring Coupled with Hydraulic Fracture Modeling in the Woodford Shale, in: All Days. Presented at the SPE Europec/EAGE Annual Conference, SPE, Copenhagen, Denmark, p. SPE-154804-MS. <https://doi.org/10.2118/154804-MS>

Nguyen, T.S., Guglielmi, Y., Graupner, B. and Rutqvist, J., 2019. Mathematical modelling of fault reactivation induced by water injection. Minerals, 9(5), p.282. <https://doi.org/10.3390/min9050282>

Nicholson, C. and Wesson, R.L., 1992. Triggered earthquakes and deep well activities. Pure and applied Geophysics, 139(3), pp.561-578. <https://doi.org/10.1007/BF00879951>

Nicholson, C., 1992, June. Earthquakes associated with deep well activities-Comments and case histories. In The 33rd US Symposium on Rock Mechanics (USRMS). OnePetro. <https://onepetro.org/ARMAUSRMS/proceedings-abstract/ARMA92/All-ARMA92/ARMA-92-1079/130500>

Nicholson, C., and Wesson, R. L., 1992. Triggered earthquakes and deep well activities. Pure and applied Geophysics, 139(3), pp.561-578. <https://doi.org/10.1007/BF00879951>

Nicholson, C., Roeloffs, E. and Wesson, R.L., 1988. The northeastern Ohio earthquake of 31 January 1986: Was it induced?. Bulletin of the Seismological Society of America, 78(1), pp.188-217. <https://doi.org/10.1785/BSSA0780010188>

Niemi, A., Bensabat, J., Joodaki, S., Basirat, F., Hedayati, M., Yang, Z., Perez, L., Levchenko, S., Shklarnik, A., Ronen, R. and Goren, Y., 2020. Characterizing CO2 residual trapping in-situ by means of single-well push-pull experiments at Heletz, Israel, pilot injection site–experimental procedures and results of the experiments. International Journal of Greenhouse Gas Control, 101, p.103129.

Niemi, A., Bensabat, J., Shtivelman, V., Edlmann, K., Gouze, P., Luquot, L., Hingerl, F., Benson, S.M., Pezard, P.A., Rasmusson, K. and Liang, T., 2016. Heletz experimental site overview, characterization and data analysis for CO2 injection and geological storage. International Journal of Greenhouse Gas Control, 48, pp.3-23. <https://doi.org/10.1016/j.ijggc.2015.12.030>

Nikulins, V., and Assinovskaya, B., 2018. Seismicity of the East Baltic region after the Kaliningrad earthquakes on 21 September 2004. Baltica, 31, pp.1.

Norbeck, J. H., and Horne, R. N., 2016. Evidence for a transient hydromechanical and frictional faulting response during the 2011 Mw 5.6 Prague, Oklahoma earthquake sequence. Journal of Geophysical Research: Solid Earth, 121(12), pp.8688-8705. <https://doi.org/10.1002/2016JB013148>

Norbeck, J. H., McClure, M. W., and Horne, R. N., 2018. Field observations at the Fenton Hill enhanced geothermal system test site support mixed-mechanism stimulation. Geothermics, 74, pp.135-149. <https://doi.org/10.1016/j.geothermics.2018.03.003>

Norbeck, J.H., McClure, M.W. and Horne, R.N., 2016. Revisiting stimulation mechanism at Fenton Hill and an investigation of the influence of fault heterogeneity on the Gutenberg-Richter b-value for rate-and-state earthquake simulations. In Proceedings of the 41st Workshop on Geothermal Reservoir Engineering (pp. 1-22). California: Stanford Univ.

Norbeck, J.H., McClure, M.W. and Horne, R.N., 2018. Field observations at the Fenton Hill enhanced geothermal system test site support mixed-mechanism stimulation. Geothermics, 74, pp.135-149. <https://doi.org/10.1016/j.geothermics.2018.03.003>

Norini, G., Carrasco-Núñez, G., Corbo-Camargo, F., Lermo, J., Rojas, J.H., Castro, C., Bonini, M., Montanari, D., Corti, G., Moratti, G. and Piccardi, L., 2019. The structural architecture of the Los Humeros volcanic complex and geothermal field. Journal of Volcanology and Geothermal Research, 381, pp.312-329. <https://doi.org/10.1016/j.jvolgeores.2019.06.010>

Ogwari, P.O. and Horton, S.P., 2016. Numerical model of pore‐pressure diffusion associated with the initiation of the 2010–2011 Guy–Greenbrier, Arkansas earthquakes. Geofluids, 16(5), pp.954-970. <https://doi.org/10.1111/gfl.12198>

Ogwari, P.O., DeShon, H.R. and Hornbach, M.J., 2018. The Dallas‐Fort Worth airport earthquake sequence: Seismicity beyond injection period. Journal of Geophysical Research: Solid Earth, 123(1), pp.553-563. <https://doi.org/10.1002/2017JB015003>

Ogwari, P.O., Horton, S.P. and Ausbrooks, S., 2016. Characteristics of induced/triggered earthquakes during the startup phase of the Guy–Greenbrier earthquake sequence in North–Central Arkansas. Seismological Research Letters, 87(3), pp.620-630. <https://doi.org/10.1785/0220150252>

Ohtake, M., 1974. Seismic activity induced by water injection at Matsushiro, Japan. Journal of Physics of the Earth, 22(1), pp.163-176. <https://doi.org/10.4294/jpe1952.22.163>

Oikawa, Y. and Yamaguchi, T., 2000. Stress measurement using rock core in an HDR field. In Proceedings of World Geothermal Congress (pp. 3819-3822).

Orzol, J., Jung, R., Jatho, R., Tischner, T., and Kehrer, P.: The GeneSys-Project: Extraction of geothermal heat from tight sediments., in: Proceedings World Geothermal Congress (pp. 24-29), April 2005.

Park, S., Kim, K.I., Xie, L., Yoo, H., Min, K.B., Kim, M., Yoon, B., Kim, K.Y., Zimmermann, G., Guinot, F. and Meier, P., 2020. Observations and analyses of the first two hydraulic stimulations in the Pohang geothermal development site, South Korea. Geothermics, 88, p.101905. <https://doi.org/10.1016/j.geothermics.2020.101905>

Park, S., Xie, L., Kim, K.I., Kwon, S., Min, K.B., Choi, J., Yoon, W.S. and Song, Y., 2017. First hydraulic stimulation in fractured geothermal reservoir in Pohang PX-2 well. Procedia Engineering, 191, pp.829-837. <https://doi.org/10.1016/j.proeng.2017.05.250>

Pechnig, R., Haverkamp, S., Wohlenberg, J., Zimmermann, G. and Burkhardt, H., 1997. Integrated log interpretation in the German Continental Deep Drilling Program: Lithology, porosity, and fracture zones. Journal of Geophysical Research: Solid Earth, 102(B8), pp.18363-18390. <https://doi.org/10.1029/96JB03802>

Pei, L., Blöcher, G., Milsch, H., Zimmermann, G., Sass, I. and Huenges, E., 2018. Thermo-mechanical properties of Upper Jurassic (Malm) carbonate rock under drained conditions. Rock Mechanics and Rock Engineering, 51(1), pp.23-45. <https://doi.org/10.1007/s00603-017-1313-0>

Peña Castro, A.F., Roth, M.P., Verdecchia, A., Onwuemeka, J., Liu, Y., Harrington, R.M., Zhang, Y. and Kao, H., 2020. Stress chatter via fluid flow and fault slip in a hydraulic fracturing‐induced earthquake sequence in the Montney Formation, British Columbia. Geophysical Research Letters, 47(14), p.e2020GL087254. <https://doi.org/10.1029/2020GL087254>

Pennington, C., Uchide, T. and Chen, X., 2022. Slip Characteristics of Induced Earthquakes: Insights from the 2015 Mw 4.0 Guthrie, Oklahoma Earthquake. Journal of Geophysical Research: Solid Earth, p.e2021JB023564. <https://doi.org/10.1029/2021JB023564>

Pérez-López, R., Mediato, J.F., Rodríguez-Pascua, M.A., Giner-Robles, J.L., Ramos, A., Martín-Velázquez, S., Martínez-Orío, R. and Fernández-Canteli, P., 2020. An active tectonic field for CO 2 storage management: the Hontomín onshore case study (Spain). Solid Earth, 11(2), pp.719-739. <https://doi.org/10.5194/se-11-719-2020>

Peter-Borie, M., Loschetter, A., Merciu, I.A., Kampfer, G. and Sigurdsson, O., 2018. Borehole damaging under thermo-mechanical loading in the RN-15/IDDP-2 deep well: towards validation of numerical modeling using logging images. Geothermal Energy, 6(1), pp.1-33. <https://doi.org/10.1186/s40517-018-0102-7>

Phillips, W. S., House, L. S., and Fehler, M. C., 1997. Detailed joint structure in a geothermal reservoir from studies of induced microearthquake clusters. Journal of Geophysical Research: Solid Earth, 102(B6), pp.11745-11763. <https://doi.org/10.1029/97JB00762>

Phillips, W. S., Rutledge, J. T., House, L. S., and Fehler, M. C., 2002. Induced microearthquake patterns in hydrocarbon and geothermal reservoirs: six case studies. In: The mechanism of induced seismicity, pp. 345-369. <https://doi.org/10.1007/978-3-0348-8179-1_15>

Phillips, W.S., House, L.S. and Fehler, M.C., 1997. Detailed joint structure in a geothermal reservoir from studies of induced microearthquake clusters. Journal of Geophysical Research: Solid Earth, 102(B6), pp.11745-11763. <https://doi.org/10.1029/97JB00762>

Phillips, W.S., Rutledge, J.T., House, L.S. and Fehler, M.C., 2002. Induced microearthquake patterns in hydrocarbon and geothermal reservoirs: six case studies. In The mechanism of induced seismicity (pp. 345-369). Birkhäuser, Basel.

Pine, R.J. and Batchelor, A.S., 1984, October. Downward migration of shearing in jointed rock during hydraulic injections. In International Journal of Rock Mechanics and Mining Sciences & Geomechanics Abstracts (Vol. 21, No. 5, pp. 249-263). Pergamon. <https://doi.org/10.1016/0148-9062(84)92681-0>

Pine, R.J., Baria, R., Pearson, R.A., Kwakwa, K. and McCartney, R., 1987. A technical summary of phase 2b of the camborne school of mines HDR project, 1983–1986. Geothermics, 16(4), pp.341-353. <https://doi.org/10.1016/0375-6505(87)90015-0>

Portier, S., Vuataz, F.D., Barrios Martinez, A.L. and Siddiqi, G., 2010. Preliminary modelling of the permeability reduction in the injection zone at Berlin geothermal field, El Salvador. In Proceedings World Geothermal Congress (Vol. 22, No. 2231, pp. 1-7). International Geothermal Association.

Prioul, R., Cornet, F.H., Dorbath, C., Dorbath, L., Ogena, M. and Ramos, E., 2000. An induced seismicity experiment across a creeping segment of the Philippine Fault. Journal of Geophysical Research: Solid Earth, 105(B6), pp.13595-13612. <https://doi.org/10.1029/2000JB900052>

Prol-Ledesma, R.M., Arango-Galvan, C. and Torres-Vera, M.A., 2016. Rigorous analysis of available data from Cerro Prieto and Las Tres Vírgenes geothermal fields with calculations for expanded electricity generation. Natural Resources Research, 25(4), pp.445-458. <https://doi.org/10.1007/s11053-016-9295-2>

Quinao, J., Sirad-Azwar, L., Clearwater, J., Hoepfinger, V., Le Brun, M. and Bardsley, C., 2013, February. Analyses and modeling of reservoir pressure changes to interpret the Rotokawa Geothermal Field response to Nga Awa Purua Power Station operation. In Proceedings of the 38th workshop on geothermal reservoir engineering. Stanford University, Stanford, California (Vol. 1113).

Quinones, L., DeShon, H.R., Jeong, S., Ogwari, P., Sufri, O., Holt, M.M. and Kwong, K.B., 2019. Tracking induced seismicity in the Fort Worth Basin: A summary of the 2008–2018 North Texas earthquake study catalog. Bulletin of the Seismological Society of America, 109(4), pp.1203-1216. <https://doi.org/10.1785/0120190057>

Quinones, L.A., DeShon, H.R., Magnani, M.B. and Frohlich, C., 2018. Stress orientations in the fort worth basin, texas, determined from earthquake focal mechanismsstress orientations in the fort worth basin. Bulletin of the Seismological Society of America, 108(3A), pp.1124-1132. <https://doi.org/10.1785/0120170337>

Raziperchikolaee, S., Kelley, M. and Gupta, N., 2018. Geomechanical characterization of a caprock-reservoir system in the Northern Appalachian Basin: Estimating spatial variation of in situ stress magnitude and orientation. Interpretation, 6(3), pp.T759-T781. <https://doi.org/10.1190/INT-2018-0068.1>

Reinecker, J., Gutmanis, J., Foxford, A., Cotton, L., Dalby, C., and Law, R., 2021. Geothermal exploration and reservoir modelling of the united downs deep geothermal project, Cornwall (UK). Geothermics, 97, pp.102226. <https://doi.org/10.1016/j.geothermics.2021.102226>

Reiter, K. and Heidbach, O., 2014. 3-D geomechanical–numerical model of the contemporary crustal stress state in the Alberta Basin (Canada). Solid Earth, 5(2), pp.1123-1149. <https://doi.org/10.5194/se-5-1123-2014>

Reiter, K., Heidbach, O., Schmitt, D., Haug, K., Ziegler, M. and Moeck, I., 2014. A revised crustal stress orientation database for Canada. Tectonophysics, 636, pp.111-124. <https://doi.org/10.1016/j.tecto.2014.08.006>

Reiter, K., Heidbach, O., Schmitt, D., Haug, K., Ziegler, M., Moeck, I., 2014. A revised crustal stress orientation database for Canada. Tectonophysics 636, 111–124. <https://doi.org/10.1016/j.tecto.2014.08.006>

Riffault, J., Dempsey, D., Archer, R., Kelkar, S. and Karra, S., 2016, February. Understanding poroelastic stressing and induced seismicity with a stochastic/deterministic model: an application to an EGS stimulation at Paralana, South Australia, 2011. In 41st Workshop on Geothermal Reservoir Engineering (pp. 22-24).

Riffault, J., Dempsey, D., Karra, S., and Archer, R., 2018. Microseismicity cloud can be substantially larger than the associated stimulated fracture volume: the case of the Paralana Enhanced Geothermal System. Journal of Geophysical Research: Solid Earth, 123(8), pp.6845-6870. <https://doi.org/10.1029/2017JB015299>

Rioseco, E. M., Reyer, D., and Schellschmidt, R., 2013. Understanding and predicting coupled hydro-mechanical fracture propagation.

Rodríguez, F.C., 2000. Hydrogeologic Model of the Geothermal Reservoir from Los Humeros, Puebla Mexico. TRANSACTIONS-GEOTHERMAL RESOURCES COUNCIL, pp.433-436.

Rodriguez, G., 2018. Reservoir Characterization of a Duvernay-Fox Creek Shale Reservoir using Seismic, Microseismic, and Well Log Data. CSEG Recorder, 43(4).

Rodríguez, V.A. and Monterossa, M., 2011. Field monitoring and management: the Berlin geothermal field case. Short Course on geothermal drilling, resource development and power plants, organized by UNU-GTP and LaGeo. El Salvador: Santa Tecla.

Rojas, A.E.O., Dussel, M. and Moeck, I., 2017. Borehole geophysical characterisation of a major fault zone in the geothermal Unterhaching Gt 2 well, South German Molasse Basin. Zeitschrift der Deutschen Gesellschaft für Geowissenschaften, 169(3), pp.445-463. 10.1127/zdgg/2017/0128

Rose, P., Sheridan, J., McCulloch, J., Moore, J. N., Kovac, K., Spielman, P., Weidler, R., and Hickman, S., 2004. The Coso EGS Project-recent developments. In Geothermal Energy: The Reliable Renewable-Geothermal Resources Council 2004 Annual Meeting, GRC, Vol. 28, pp.227-231.

Rubinstein, J.L., Ellsworth, W.L. and McGarr, A., 2012, December. The 2001-present triggered seismicity sequence in the Raton basin of southern Colorado/Northern New Mexico. In AGU Fall Meeting Abstracts (Vol. 2012, pp. S34A-02). <https://ui.adsabs.harvard.edu/abs/2012AGUFM.S34A..02R/abstract>

Rubinstein, J.L., Ellsworth, W.L., McGarr, A. and Benz, H.M., 2014. The 2001–present induced earthquake sequence in the Raton Basin of northern New Mexico and southern Colorado. Bulletin of the Seismological Society of America, 104(5), pp.2162-2181. <https://doi.org/10.1785/0120140009>

Ruiz-Barajas, S., Sharma, N., Convertito, V., Zollo, A. and Benito, B., 2017. Temporal evolution of a seismic sequence induced by a gas injection in the Eastern coast of Spain. Scientific reports, 7(1), pp.1-15. <https://doi.org/10.1038/s41598-017-02773-2>

Rummel, F. and Klee, G., 1995. State of stress at the European HDR candidate sites Urach and Soultz. In World Geothermal Congress. City: International Geothermal Association: Florence, Italy (pp. 2639-2642).

Rutledge, J.T., Phillips, W.S., 2003. Case History Hydraulic stimulation of natural fractures as revealed by induced microearthquakes , Carthage Cotton Valley gas field , east Texas 68, 441–452. <https://doi.org/10.1190/1.1567214>

Rutqvist, J., 2012. The geomechanics of CO2 storage in deep sedimentary formations. Geotechnical and Geological Engineering, 30(3), pp.525-551. <https://doi.org/10.1007/s10706-011-9491-0>

Rutqvist, J., Dobson, P.F., Garcia, J., Hartline, C., Jeanne, P., Oldenburg, C.M., Vasco, D.W. and Walters, M., 2015. The northwest Geysers EGS demonstration project, California: Pre-stimulation modeling and interpretation of the stimulation. Mathematical Geosciences, 47(1), pp.3-29. <https://doi.org/10.1007/s11004-013-9493-y>

Rutqvist, J., Vasco, D.W. and Myer, L., 2010. Coupled reservoir-geomechanical analysis of CO2 injection and ground deformations at In Salah, Algeria. International Journal of Greenhouse Gas Control, 4(2), pp.225-230. <https://doi.org/10.1016/j.ijggc.2009.10.017>

Ryan, B. E.: Petrophysical Properties of the Woodford Formation in the Ardmore Basin in Oklahoma, U.S.A, The University of Texas at Arlington, 101 pp., 2017.

Ryan, B., 2017. Petrophysical properties of the Woodford Formation in the Ardmore Basin in Oklahoma, USA (Doctoral dissertation).

Sahara, D., Meller, C. and Kohl, T., 2016. Characterization of the geomechanical properties of a reservoir rock from an integrated analysis of borehole data.

Sasaki, S. and Kaieda, H., 1998. Stress state at the Hijiori HDR site inferred from focal mechanism data. In 4th Int. HDR Forum Strasbourg.

Sasaki, S., 1998. Characteristics of microseismic events induced during hydraulic fracturing experiments at the Hijiori hot dry rock geothermal energy site, Yamagata, Japan. Tectonophysics, 289(1-3), pp.171-188. <https://doi.org/10.1016/S0040-1951(97)00314-4>

Sattler, F. R.: Lithologic Properties of the Upper Ordovician Utica Formation , Michigan Basin , USA : A Geological Characterization and Assessment of Carbon Dioxide Confinement Potential, Western Michigan University, 103 pp., 2015.

Sausse, J., Fourar, M. and Genter, A., 2006. Permeability and alteration within the Soultz granite inferred from geophysical and flow log analysis. Geothermics, 35(5-6), pp.544-560. <https://doi.org/10.1016/j.geothermics.2006.07.003>

Savage, D., Cave, M.R., Milodowski, A.E. and George, I., 1987. Hydrothermal alteration of granite by meteoric fluid: an example from the Carnmenellis Granite, United Kingdom. Contributions to Mineralogy and Petrology, 96(3), pp.391-405. <https://doi.org/10.1007/BF00371257>

Scales, M.M., DeShon, H.R., Magnani, M.B., Walter, J.I., Quinones, L., Pratt, T.L. and Hornbach, M.J., 2017. A decade of induced slip on the causative fault of the 2015 Mw 4.0 Venus earthquake, northeast Johnson County, Texas. Journal of Geophysical Research: Solid Earth, 122(10), pp.7879-7894. <https://doi.org/10.1002/2017JB014460>

Schindler, A., Jurado, M.J. and Müller, B., 1998. Stress orientation and tectonic regime in the northwestern Valencia Trough from borehole data. Tectonophysics, 300(1-4), pp.63-77. <https://doi.org/10.1016/S0040-1951(98)00234-0>

Schindler, M., Baumgärtner, J., Gandy, T., Hauffe, P., Hettkamp, T., Menzel, H., Penzkofer, P., Teza, D., Tischner, T. and Wahl, G., 2010, April. Successful hydraulic stimulation techniques for electric power production in the Upper Rhine Graben, Central Europe. In Proceedings World geothermal congress (Vol. 2010).

Schmittbuhl, J., Lambotte, S., Lengliné, O., Grunberg, M., Jund, H., Vergne, J., Cornet, F., Doubre, C. and Masson, F., 2021. Induced and triggered seismicity below the city of Strasbourg, France from November 2019 to January 2021. Comptes Rendus. Géoscience, 353(S1), pp.561-584. 10.5802/crgeos.71

Schmittbuhl, J., Lambotte, S., Lengliné, O., Grunberg, M., Jund, H., Vergne, J., Cornet, F., Doubre, C., and Masson, F., 2021. Induced and triggered seismicity below the city of Strasbourg, France from November 2019 to January 2021. Comptes Rendus. Géoscience, 353(S1), pp.1-24. https://doi.org/10.5802/crgeos.71

Schoenball, M., 2014. Evolution of stress and seismicity in fractured geothermal reservoirs.

Schoenball, M., Walsh, F.R., Weingarten, M. and Ellsworth, W.L., 2018. How faults wake up: the Guthrie-Langston, Oklahoma earthquakes. The Leading Edge, 37(2), pp.100-106. <https://doi.org/10.1190/tle37020100.1>

Schultz, R., Ellsworth, W.L. and Beroza, G.C., 2022. Statistical bounds on how induced seismicity stops. Scientific reports, 12(1), pp.1-11. <https://doi.org/10.1038/s41598-022-05216-9>

Schultz, R., Mei, S., Pană, D., Stern, V., Gu, Y.J., Kim, A., Eato, D., 2015. The cardston earthquake swarm and hydraulic fracturing of the exshaw formation (Alberta bakken play). Bulletin of the Seismological Society of America 105, 2871–2884. <https://doi.org/10.1785/0120150131>

Schultz, R., Skoumal, R.J., Brudzinski, M.R., Eaton, D., Baptie, B., Ellsworth, W., 2020. Hydraulic fracturing‐induced seismicity. Reviews of Geophysics 58, 1–43. <https://doi.org/10.1029/2019RG000695>

Schultz, R., Stern, V., Novakovic, M., Atkinson, G. and Gu, Y.J., 2015. Hydraulic fracturing and the Crooked Lake Sequences: Insights gleaned from regional seismic networks. Geophysical Research Letters, 42(8), pp.2750-2758. <https://doi.org/10.1002/2015GL063455>

Schultz, R., Wang, R., Gu, Y.J., Haug, K. and Atkinson, G., 2017. A seismological overview of the induced earthquakes in the Duvernay play near Fox Creek, Alberta. Journal of Geophysical Research: Solid Earth, 122(1), pp.492-505. <https://doi.org/10.1002/2016JB013570>

Scibek, J., 2020. Multidisciplinary database of permeability of fault zones and surrounding protolith rocks at world-wide sites. Scientific Data, 7(1), pp.1-14. <https://doi.org/10.1038/s41597-020-0435-5>

Seeber, L., Armbruster, J.G. and Kim, W.Y., 2004. A fluid-injection-triggered earthquake sequence in Ashtabula, Ohio: Implications for seismogenesis in stable continental regions. Bulletin of the Seismological Society of America, 94(1), pp.76-87. <https://doi.org/10.1785/0120020091>

Selvadurai, P., Selvadurai, P.A. and Nejati, M., 2019. A multi-phasic approach for estimating the Biot coefficient for Grimsel granite. Solid Earth, 10(6), pp.2001-2014. https://doi.org/10.5194/se-10-2001-2019

Shen, L.W., Schmitt, D.R. and Haug, K., 2019. Quantitative constraints to the complete state of stress from the combined borehole and focal mechanism inversions: Fox Creek, Alberta. Tectonophysics, 764, pp.110-123. <https://doi.org/10.1016/j.tecto.2019.04.023>

Shen, L.W., Schmitt, D.R., Haug, K., 2018. Measurements of the States of In Situ Stress for the Duvernay Formation near Fox Creek, West-Central Alberta, Alberta Energy Regulator/Alberta Geological Survey, AER/AGS Report.

Shen, L.W., Schmitt, D.R., Wang, R. and Hauck, T.E., 2021. States of in situ stress in the Duvernay East Shale Basin and Willesden Green of Alberta, Canada: Variable in situ stress states effect fault stability. Journal of Geophysical Research: Solid Earth, 126(6), p.e2020JB021221. <https://doi.org/10.1029/2020JB021221>

Sherburn, S., Bromley, C., Bannister, S., Sewell, S. and Bourguignon, S., 2015, April. New Zealand geothermal induced seismicity: an overview. In Proceedings of the World Geothermal Congress.

Sherburn, S., Sewell, S.M., Bourguignon, S., Cumming, W., Bannister, S., Bardsley, C., Winick, J., Quinao, J. and Wallis, I.C., 2015. Microseismicity at rotokawa geothermal field, New Zealand, 2008–2012. Geothermics, 54, pp.23-34. <https://doi.org/10.1016/j.geothermics.2014.11.001>

Shin, K., Ito, H. and Oikawa, Y., 2000. Stress state at the Ogachi site. In Proceedings (pp. 1749-1752).

Shirzaei, M., Ellsworth, W.L., Tiampo, K.F., González, P.J. and Manga, M., 2016. Surface uplift and time-dependent seismic hazard due to fluid injection in eastern Texas. Science, 353(6306), pp.1416-1419. <https://www.science.org/doi/abs/10.1126/science.aag0262>

Shirzaei, M., Manga, M. and Zhai, G., 2019. Hydraulic properties of injection formations constrained by surface deformation. Earth and Planetary Science Letters, 515, pp.125-134. <https://doi.org/10.1016/j.epsl.2019.03.025>

Siratovich, P.A., Davidson, J., Villeneuve, M., Gravley, D., Kennedy, B., Cole, J., Wyering, L. and Price, L., 2012, November. Physical and mechanical properties of the Rotokawa Andesite from production wells RK 27\_L2, RK28 and RK30. In New Zealand Geothermal Workshop 2012 Proceedings (pp. 19-21).

Siratovich, P.A., Heap, M.J., Villeneuve, M.C., Cole, J.W., Kennedy, B.M., Davidson, J. and Reuschlé, T., 2016. Mechanical behaviour of the Rotokawa Andesites (New Zealand): Insight into permeability evolution and stress-induced behaviour in an actively utilised geothermal reservoir. Geothermics, 64, pp.163-179. <https://doi.org/10.1016/j.geothermics.2016.05.005>

Siratovich, P.A., Heap, M.J., Villenueve, M.C., Cole, J.W. and Reuschlé, T., 2014. Physical property relationships of the Rotokawa Andesite, a significant geothermal reservoir rock in the Taupo Volcanic Zone, New Zealand. Geothermal Energy, 2(1), pp.1-31. <https://doi.org/10.1186/s40517-014-0010-4>

Siratovich, P.A., von Aulock, F.W., Lavallée, Y., Cole, J.W., Kennedy, B.M. and Villeneuve, M.C., 2015. Thermoelastic properties of the Rotokawa Andesite: a geothermal reservoir constraint. Journal of Volcanology and Geothermal Research, 301, pp.1-13. <https://doi.org/10.1016/j.jvolgeores.2015.05.003>

Sisi, A.A., Schlittenhardt, J. and Spies, T., 2017. Investigation of Non-Stationarity Associated with Induced Seismicity and Its Implication in Probabilistic Seismic Hazard Analysis. D-A-CH-Tagung: Erdbebeningenieurwesen und Baudynamik.

Skoumal, R.J., Barbour, A.J., Brudzinski, M.R., Langenkamp, T. and Kaven, J.O., 2020. Induced seismicity in the Delaware basin, Texas. Journal of Geophysical Research: Solid Earth, 125(1), p.e2019JB018558. <https://doi.org/10.1029/2019JB018558>

Skoumal, R.J., Brudzinski, M.R. and Currie, B.S., 2015. Earthquakes induced by hydraulic fracturing in Poland Township, Ohio. Bulletin of the Seismological Society of America, 105(1), pp.189-197. <https://doi.org/10.1785/0120140168>

Smye, K.M., Lemons, C.R., Eastwood, R., McDaid, G. and Hennings, P.H., 2019. Stratigraphic architecture and petrophysical characterization of formations for deep disposal in the Fort Worth Basin, Texas. Interpretation, 7(4), pp.SL1-SL17. <https://doi.org/10.1190/INT-2018-0195.1>

Soltanzadeh, M., Davis, G., Fox, A., Hume, D., Rahim, N., 2015. Application of Mechanical and Mineralogical Rock Properties to Identify Fracture Fabrics in the Devonian Duvernay Formation in Alberta 1668–1681. <https://doi.org/10.15530/urtec-2015-2178289>

Somerton, W.H., 1980. Some physical properties of Cerro Prieto cores. Geothermics, 9(1-2), pp.159-168. <https://doi.org/10.1016/0375-6505(80)90029-2>

Sone, H. and Zoback, M.D., 2013. Mechanical properties of shale-gas reservoir rocks—Part 1: Static and dynamic elastic properties and anisotropy. Geophysics, 78(5), pp.D381-D392. <https://doi.org/10.1190/geo2013-0050.1>

Sone, H., Zoback, M.D., 2013. Mechanical properties of shale-gas reservoir rocks — Part 1: Static and dynamic elastic properties and anisotropy. GEOPHYSICS 78, D381--D392. <https://doi.org/10.1190/geo2013-0050.1>

Sonnenthal, E., Spycher, N., Callahan, O., Cladouhos, T. and Petty, S., 2012. A thermal–hydrological–chemical model for the enhanced geothermal system demonstration project at Newberry Volcano, Oregon. In Proceedings of the 37th Workshop on Geothermal Reservoir Engineering, Stanford, CA (Vol. 30).

Srinivasan, K., Dean, B., Belobraydic, M., Azmi, Z., 2013. Evolution of horizontal well hydraulic fracturing in the Granite Wash - Understanding well performance drivers of a liquids-rich Anadarko basin formation. Society of Petroleum Engineers - SPE Hydraulic Fracturing Technology Conference 2013 463–488. <https://doi.org/10.2118/163857-ms>

Stabile, T.A., Giocoli, A., Perrone, A., Piscitelli, S. and Lapenna, V., 2014. Fluid injection induced seismicity reveals a NE dipping fault in the southeastern sector of the High Agri Valley (southern Italy). Geophysical Research Letters, 41(16), pp.5847-5854. <https://doi.org/10.1002/2014GL060948>

State studying link between fracking, Lawrence County earthquakes: https://www.post-gazette.com/business/powersource/2016/04/29/State-studying-link-between-fracking-and-Lawrence-County-earthquakes/stories/201604290099, last access: 3 June 2022.

Stober, I., 2011. Depth-and pressure-dependent permeability in the upper continental crust: data from the Urach 3 geothermal borehole, southwest Germany. Hydrogeology Journal, 19(3), pp.685-699. <https://doi.org/10.1007/s10040-011-0704-7>

Stork, A.L., Verdon, J.P. and Kendall, J.M., 2015. The microseismic response at the In Salah Carbon Capture and Storage (CCS) site. International Journal of Greenhouse Gas Control, 32, pp.159-171. <https://doi.org/10.1016/j.ijggc.2014.11.014>

Sumy, D.F., Cochran, E.S., Keranen, K.M., Wei, M. and Abers, G.A., 2014. Observations of static Coulomb stress triggering of the November 2011 M5. 7 Oklahoma earthquake sequence. Journal of Geophysical Research: Solid Earth, 119(3), pp.1904-1923. <https://doi.org/10.1002/2013JB010612>

Sun, X., and Hartzell, S., 2014. Finite‐fault slip model of the 2011 Mw 5.6 Prague, Oklahoma earthquake from regional waveforms. Geophysical Research Letters, 41(12), pp.4207-4213. <https://doi.org/10.1002/2014GL060410>

Sundberg, J., Back, P.E., Christiansson, R., Hökmark, H., Ländell, M. and Wrafter, J., 2009. Modelling of thermal rock mass properties at the potential sites of a Swedish nuclear waste repository. International Journal of Rock Mechanics and Mining Sciences, 46(6), pp.1042-1054. <https://doi.org/10.1016/j.ijrmms.2009.02.004>

Surma, F. and Geraud, Y., 2003. Porosity and thermal conductivity of the Soultz-sous-Forêts granite. Pure and Applied Geophysics, 160(5), pp.1125-1136. <https://doi.org/10.1007/PL00012564>

Tadokoro, K., Ando, M. and Nishigami, K.Y., 2000. Induced earthquakes accompanying the water injection experiment at the Nojima fault zone, Japan: seismicity and its migration. Journal of Geophysical Research: Solid Earth, 105(B3), pp.6089-6104. <https://doi.org/10.1029/1999JB900416>

Taherynia, M.H., Fatemi Aghda, S.M. and Fahimifar, A., 2016. In-situ stress state and tectonic regime in different depths of earth crust. Geotechnical and Geological Engineering, 34(2), pp.679-687. <https://doi.org/10.1007/s10706-016-9978-9>

Tan, Y., Hu, J., Zhang, H., Chen, Y., Qian, J., Wang, Q., Zha, H., Tang, P. and Nie, Z., 2020. Hydraulic fracturing induced seismicity in the southern Sichuan Basin due to fluid diffusion inferred from seismic and injection data analysis. Geophysical Research Letters, 47(4), p.e2019GL084885. <https://doi.org/10.1029/2019GL084885>

Tang, X., Jiang, Z., Song, Y., Luo, Q., Li, Z., Wang, G. and Wang, X., 2021. Advances on the mechanism of reservoir forming and gas accumulation of the Longmaxi Formation shale in Sichuan Basin, China. Energy & Fuels, 35(5), pp.3972-3988. <https://doi.org/10.1021/acs.energyfuels.0c04204>

Teklu, T.W., Park, D., Jung, H. and Miskimins, J.L., 2018, September. Integrated rock characterization of a shale gas field in the Horn River Basin, Canada. In Unconventional Resources Technology Conference, Houston, Texas, 23-25 July 2018 (pp. 512-542). Society of Exploration Geophysicists, American Association of Petroleum Geologists, Society of Petroleum Engineers. <https://doi.org/10.15530/urtec-2018-2880467>

Teklu, T.W., Park, D., Jung, H., Miskimins, J.L., 2018. Integrated rock characterization of a shale gas field in the Horn River Basin, Canada. SPE/AAPG/SEG Unconventional Resources Technology Conference 2018, URTC 2018. <https://doi.org/10.15530/urtec-2018-2880467>

Tenma, N., Yamaguchi, T. and Zyvoloski, G., 2008. The Hijiori hot dry rock test site, Japan: evaluation and optimization of heat extraction from a two-layered reservoir. Geothermics, 37(1), pp.19-52. <https://doi.org/10.1016/j.geothermics.2007.11.002>

Tenzer, H., Park, C.H., Kolditz, O. and McDermott, C.I., 2010. Application of the geomechanical facies approach and comparison of exploration and evaluation methods used at Soultz-sous-Forêts (France) and Spa Urach (Germany) geothermal sites. Environmental Earth Sciences, 61(4), pp.853-880. <https://doi.org/10.1007/s12665-009-0403-z>

Thorpe, S., 2017. Time series analysis of surface deformation associated with fluid injection and induced seismicity in Timpson, Texas using DInSAR methods.

Thorpe, S.:Time series analysis of surface deformation associated with fluid injection and induced seismicity in Timpson, Texas using DInSAR methods. Master dissertation, University of Western Ontario, Canada, 155 pp., 2017. <https://ir.lib.uwo.ca/etd/5126/>

Tischner, T., Krug, S., Pechan, E., Hesshaus, A., Jatho, R., Bischoff, M., and Wonik, T.: Massive hydraulic fracturing in low permeable sedimentary rock in the GeneSys project, in: Proceedings Thirty-Eights Workshop on Geothermal Reservoir Engineering, SGP-TR-198, Stanford University, Stanford, California (pp. 11-13), February 2013.

Trugman, D.T., Borsa, A.A. and Sandwell, D.T., 2014. Did stresses from the Cerro Prieto Geothermal Field influence the El Mayor‐Cucapah rupture sequence?. Geophysical Research Letters, 41(24), pp.8767-8774. <https://doi.org/10.1002/2014GL061959>

Tung, S., Zhai, G. and Shirzaei, M., 2021. Potential link between 2020 Mentone, West Texas M5 earthquake and nearby wastewater injection: Implications for aquifer mechanical properties. Geophysical Research Letters, 48(3), p.e2020GL090551. <https://doi.org/10.1029/2020GL090551>

Urban, E. and Lermo, J.F., 2013, February. Local seismicity in the exploitation of Los Humeros geothermal field, Mexico. In 38th Workshop on Geothermal Reservoir Engineering (pp. 11-13).

Urbancic, T. I., Shumila, V., Rutledge, J. T., and Zinno, R. J.: Determining hydraulic fracture behavior using microseismicity, Vail Rocks 1999, The 37th U.S. Symposium on Rock Mechanics (USRMS), ARMA--99--0991, 1999.

Urbancic, T.I., Rutledge, J., 2000. Using microseismicity to map cotton valley hydraulic fractures, in: SEG Technical Program Expanded Abstracts 2000. Society of Exploration Geophysicists, pp. 1444–1448. <https://doi.org/10.1190/1.1815676>

Vaisblat, N., Shokri, A.R., Ayranci, K., Harris, N., Chalaturnyk, R.J., 2019. Significance of rock compositional control on geomechanical properties and hydraulic fracturing of the montney formation, Western Canadian Basin. SPE/AAPG/SEG Asia Pacific Unconventional Resources Technology Conference 2019, APUR 2019. <https://doi.org/10.15530/ap-urtec-2019-198199>

Valès, F., Minh, D.N., Gharbi, H. and Rejeb, A., 2004. Experimental study of the influence of the degree of saturation on physical and mechanical properties in Tournemire shale (France). Applied Clay Science, 26(1-4), pp.197-207. <https://doi.org/10.1016/j.clay.2003.12.032>

Valley, B. and Evans, K.F., 2007, January. Stress state at Soultz-sous-Forêts to 5 km depth from wellbore failure and hydraulic observations. In Proceedings, 32nd workshop on geothermal reservoir engineering (pp. 17481-17469).

Valley, B. and Evans, K.F., 2009. Stress orientation to 5 km depth in the basement below Basel (Switzerland) from borehole failure analysis. Swiss Journal of Geosciences, 102(3), pp.467-480. <https://doi.org/10.1007/s00015-009-1335-z>

Valley, B. and Evans, K.F., 2019. Stress magnitudes in the Basel enhanced geothermal system. International Journal of Rock Mechanics and Mining Sciences, 118, pp.1-20. <https://doi.org/10.1016/j.ijrmms.2019.03.008>

Valley, B., and Evans, K. F.: Stress state at Soultz-sous-Forêts to 5 km depth from wellbore failure and hydraulic observations, in: Proceedings, 32nd workshop on geothermal reservoir engineering (pp. 17481-17469), January 2007.

Van Poollen, H.K. and Hoover, D.B., 1970. Waste disposal and earthquakes at the rocky mountain arsenal, Derby, Colorado. Journal of Petroleum Technology, 22(08), pp.983-993. <https://doi.org/10.2118/2558-PA>

Verdecchia, A., Wang, B., Liu, Y., Harrington, R., Roth, M., Castro, A.P. and Onwuemeka, J., 2020. Exploring possible causative mechanisms for earthquakes triggered by hydraulic fracturing: examples from the Montney Basin, BC, Canada (No. EGU2020-10680). Copernicus Meetings. <https://doi.org/10.5194/egusphere-egu2020-10680>

Verdon, J.P., Stork, A.L., Bissell, R.C., Bond, C.E. and Werner, M.J., 2015. Simulation of seismic events induced by CO2 injection at In Salah, Algeria. Earth and Planetary Science Letters, 426, pp.118-129. <https://doi.org/10.1016/j.epsl.2015.06.029>

Vidal, J. and Genter, A., 2018. Overview of naturally permeable fractured reservoirs in the central and southern Upper Rhine Graben: Insights from geothermal wells. Geothermics, 74, pp.57-73. <https://doi.org/10.1016/j.geothermics.2018.02.003>

Vilarrasa, V., Makhnenko, R.Y. and Rutqvist, J., 2019. Field and laboratory studies of geomechanical response to the injection of CO2. In Science of carbon storage in deep saline formations (pp. 209-236). Elsevier. <https://doi.org/10.1016/B978-0-12-812752-0.00009-5>

Vilarrasa, V., Rinaldi, A.P. and Rutqvist, J., 2017. Long-term thermal effects on injectivity evolution during CO2 storage. International Journal of Greenhouse Gas Control, 64, pp.314-322. <https://doi.org/10.1016/j.ijggc.2017.07.019>

Vilarrasa, V., Rutqvist, J. and Rinaldi, A.P., 2015. Thermal and capillary effects on the caprock mechanical stability at In Salah, Algeria. Greenhouse Gases: Science and Technology, 5(4), pp.449-461. <https://doi.org/10.1002/ghg.1486>

Villaseñor, A., Herrmann, R.B., Gaite, B. and Ugalde, A., 2020. Fault reactivation by gas injection at an underground gas storage off the east coast of Spain. Solid Earth, 11(1), pp.63-74. <https://doi.org/10.5194/se-11-63-2020>

Villeneuve, M.C., Heap, M.J., Kushnir, A.R., Qin, T., Baud, P., Zhou, G. and Xu, T., 2018. Estimating in situ rock mass strength and elastic modulus of granite from the Soultz-sous-Forêts geothermal reservoir (France). Geothermal Energy, 6(1), pp.1-29. <https://doi.org/10.1186/s40517-018-0096-1>

Villiger, L., Gischig, V.S., Doetsch, J., Krietsch, H., Dutler, N.O., Jalali, M., Valley, B., Selvadurai, P.A., Mignan, A., Plenkers, K. and Giardini, D., 2020. Influence of reservoir geology on seismic response during decameter-scale hydraulic stimulations in crystalline rock. Solid Earth, 11(2), pp.627-655. <https://doi.org/10.5194/se-11-627-2020>

Wakahama, H., Mitoa, S., Ohsumi, T., Ueda, A., Yajima, T., Satoh, H., Sugiyama, K., Ozawa, A., Ajima, S., Todaka, N. and Sato, T., 2009. A concept of CO2 Georeactor sequestration at the Ogachi HDR site, NE Japan. Energy Procedia, 1(1), pp.3683-3689. <https://doi.org/10.1016/j.egypro.2009.02.166>

Wallroth, T., Eliasson, T., and Sundquist, U., 1999. Hot dry rock research experiments at Fjällbacka, Sweden. Geothermics, 28(4-5), pp.617-625. <https://doi.org/10.1016/S0375-6505(99)00032-2>

Walsh III, F. R., and Zoback, M. D., 2016. Probabilistic assessment of potential fault slip related to injection-induced earthquakes: Application to north-central Oklahoma, USA. Geology, 44(12), pp.991-994. <https://doi.org/10.1130/G38275.1>

Walter, J.I., Dotray, P.J., Frohlich, C. and Gale, J.F., 2016. Earthquakes in northwest Louisiana and the Texas–Louisiana border possibly induced by energy resource activities within the Haynesville Shale Play. Seismological Research Letters, 87(2A), pp.285-294. <https://doi.org/10.1785/0220150193>

Walter, J.I., Frohlich, C., Borgfeldt, T., 2018. Natural and induced seismicity in the Texas and Oklahoma panhandles. Seismological Research Letters 89, 2437–2446. <https://doi.org/10.1785/0220180105>

Wang, B., Harrington, R.M., Liu, Y., Kao, H. and Yu, H., 2020. A study on the largest hydraulic‐fracturing‐induced earthquake in Canada: Observations and static stress‐drop estimation. Bulletin of the Seismological Society of America, 110(5), pp.2283-2294. <https://doi.org/10.1785/0120190261>

Wang, B., Verdecchia, A., Kao, H., Harrington, R.M., Liu, Y. and Yu, H., 2021. A study on the largest hydraulic fracturing induced earthquake in Canada: Numerical modeling and triggering mechanism. Bulletin of the Seismological Society of America, 111(3), pp.1392-1404. <https://doi.org/10.1785/0120200251>

Wang, J., Li, T., Gu, Y.J., Schultz, R., Yusifbayov, J. and Zhang, M., 2020. Sequential fault reactivation and secondary triggering in the March 2019 Red Deer induced earthquake swarm. Geophysical Research Letters, 47(22), p.e2020GL090219. <https://doi.org/10.1029/2020GL090219>

Wang, K., Ellsworth, W. and Beroza, G.C., 2020. Revisiting the Timpson induced earthquake sequence: A system of two parallel faults. Geophysical Research Letters, 47(15), p.e2020GL089192. <https://doi.org/10.1029/2020GL089192>

Wang, L., Kwiatek, G., Rybacki, E., Bohnhoff, M. and Dresen, G., 2020. Injection‐induced seismic moment release and laboratory fault slip: Implications for fluid‐induced seismicity. Geophysical Research Letters, 47(22), p.e2020GL089576. <https://doi.org/10.1029/2020GL089576>

Wang, L., Kwiatek, G., Rybacki, E., Bonnelye, A., Bohnhoff, M. and Dresen, G., 2020. Laboratory study on fluid‐induced fault slip behavior: The role of fluid pressurization rate. Geophysical Research Letters, 47(6), p.e2019GL086627. <https://doi.org/10.1029/2019GL086627>

Wang, R., Gu, Y.J., Schultz, R., Kim, A. and Atkinson, G., 2016. Source analysis of a potential hydraulic‐fracturing‐induced earthquake near Fox Creek, Alberta. Geophysical Research Letters, 43(2), pp.564-573. <https://doi.org/10.1002/2015GL066917>

Weir, R.M., Eaton, D.W., Lines, L.R., Lawton, D.C. and Ekpo, E., 2018. Inversion and interpretation of seismic-derived rock properties in the Duvernay play. Interpretation, 6(2), pp.SE1-SE14. <https://doi.org/10.1190/INT-2017-0149.1>

Westaway, R., 2017. Integrating induced seismicity with rock mechanics: a conceptual model for the 2011 Preese Hall fracture development and induced seismicity. Geological Society, London, Special Publications, 454(1), pp.327-359. <https://doi.org/10.1144/SP454.12>

Williams‐Stroud, S., Bauer, R., Leetaru, H., Oye, V., Stanek, F., Greenberg, S. and Langet, N., 2020. Analysis of microseismicity and reactivated fault size to assess the potential for felt events by CO2 injection in the Illinois Basin. Bulletin of the Seismological Society of America, 110(5), pp.2188-2204. <https://doi.org/10.1785/0120200112>

Wolfgramm, M., Bartels, J., Hoffmann, F., Kittl, G., Lenz, G., Seibt, P., Schulz, R., Thomas, R. and Unger, H.J., 2007, May. Unterhaching geothermal well doublet: structural and hydrodynamic reservoir characteristic; Bavaria (Germany). In European Geothermal Congress (Vol. 30).

Wolfgramm, M., Bloch, T., Bartels, J., Heuberger, S., Kuhn, P., Naef, H., Voigt, H.D., Seibt, P., Sonderegger, M., Steiger, T. and Uhlig, S., 2015. Reservoir-geological characterization of a fractured limestone: Results obtained from the geothermal well St. Gallen GT-1 (Switzerland).

Wolhart, S.L., Harting, T.A., Dahlem, J.E., Young, T., Mayerhofer, M.J., Lolon, E.P., 2006. Hydraulic Fracture Diagnostics Used To Optimize Development in the Jonah Field, in: All Days. Presented at the SPE Annual Technical Conference and Exhibition, SPE, San Antonio, Texas, USA, p. SPE-102528-MS. <https://doi.org/10.2118/102528-MS>

Woo, J.U., Kim, M., Sheen, D.H., Kang, T.S., Rhie, J., Grigoli, F., Ellsworth, W.L. and Giardini, D., 2019. An in‐depth seismological analysis revealing a causal link between the 2017 MW 5.5 Pohang earthquake and EGS project. Journal of Geophysical Research: Solid Earth, 124(12), pp.13060-13078. <https://doi.org/10.1029/2019JB018368>

Wu, Q., Chen, X. and Abercrombie, R.E., 2019. Source complexity of the 2015 Mw 4.0 Guthrie, Oklahoma earthquake. Geophysical Research Letters, 46(9), pp.4674-4684. <https://doi.org/10.1029/2019GL082690>

Wyering, L.D., Villeneuve, M.C., Wallis, I.C., Siratovich, P.A., Kennedy, B.M., Gravley, D.M. and Cant, J.L., 2014. Mechanical and physical properties of hydrothermally altered rocks, Taupo Volcanic Zone, New Zealand. Journal of Volcanology and Geothermal Research, 288, pp.76-93. <https://doi.org/10.1016/j.jvolgeores.2014.10.008>

Xie, L., Min, K. B., and Song, Y., 2015. Observations of hydraulic stimulations in seven enhanced geothermal system projects. Renewable Energy, 79, pp.56-65. <https://doi.org/10.1016/j.renene.2014.07.044>

Xu, S., Liu, R., Hao, F., Engelder, T., Yi, J., Zhang, B. and Shu, Z., 2019. Complex rotation of maximum horizontal stress in the Wufeng-Longmaxi Shale on the eastern margin of the Sichuan Basin, China: Implications for predicting natural fractures. Marine and Petroleum Geology, 109, pp.519-529. <https://doi.org/10.1016/j.marpetgeo.2019.06.008>

Yang, F., Babarinde, O., Okwen, R., Frailey, S. and Whittaker, S., 2018, October. Modeling commercial-scale CO2 injection in Mt. Simon Sandstone near Decatur, IL storage sites. In 14th Greenhouse Gas Control Technologies Conference Melbourne (pp. 21-26).

Yang, H., Zhou, P., Fang, N., Zhu, G., Xu, W., Su, J., 2020. A Shallow Shock : The 25 February 2019 M L 4 . 9 Earthquake in the Weiyuan Shale Gas Field in Sichuan , China. <https://doi.org/10.1785/0220200202.Supplemental>

Yang, H., Zhou, P., Fang, N., Zhu, G., Xu, W., Su, J., Meng, F. and Chu, R., 2020. A shallow shock: the 25 February 2019 ML 4.9 earthquake in the Weiyuan shale gas field in Sichuan, China. Seismological Society of America, 91(6), pp.3182-3194. <https://doi.org/10.1785/0220200202>

Yeck, W. L., Hayes, G. P., McNamara, D. E., Rubinstein, J. L., Barnhart, W. D., Earle, P. S., and Benz, H. M., 2017. Oklahoma experiences largest earthquake during ongoing regional wastewater injection hazard mitigation efforts. Geophysical Research Letters, 44(2), pp.711-717. <https://doi.org/10.1002/2016GL071685>

Yeck, W. L., Weingarten, M., Benz, H. M., McNamara, D. E., Bergman, E. A., Herrmann, R. B., Rubinstein, J. L., and Earle, P. S., 2016. Far‐field pressurization likely caused one of the largest injection induced earthquakes by reactivating a large preexisting basement fault structure. Geophysical Research Letters, 43(19), pp.10-198. <https://doi.org/10.1002/2016GL070861>

Yeck, W.L., Weingarten, M., Benz, H.M., McNamara, D.E., Bergman, E.A., Herrmann, R.B., Rubinstein, J.L. and Earle, P.S., 2016. Far‐field pressurization likely caused one of the largest injection induced earthquakes by reactivating a large preexisting basement fault structure. Geophysical Research Letters, 43(19), pp.10-198. <https://doi.org/10.1002/2016GL070861>

Yehya, A., Yang, Z. and Rice, J.R., 2018. Effect of fault architecture and permeability evolution on response to fluid injection. Journal of Geophysical Research: Solid Earth, 123(11), pp.9982-9997. <https://doi.org/10.1029/2018JB016550>

Yeo, I.W., Brown, M.R.M., Ge, S. and Lee, K.K., 2020. Causal mechanism of injection-induced earthquakes through the Mw 5.5 Pohang earthquake case study. Nature communications, 11(1), pp.1-12. <https://doi.org/10.1038/s41467-020-16408-0>

Yoon, C.E., Huang, Y., Ellsworth, W.L. and Beroza, G.C., 2017. Seismicity during the initial stages of the Guy‐Greenbrier, Arkansas, earthquake sequence. Journal of Geophysical Research: Solid Earth, 122(11), pp.9253-9274. <https://doi.org/10.1002/2017JB014946>

Yu, W., 2017. Laboratory Geomechanical Characterization of the Arbuckle Group and Crystalline Basement Rocks in Oklahoma.

Yu, W.: Laboratory Geomechanical Characterization of the Arbuckle Group and Crystalline Basement Rocks in Oklahoma. Master dissertation, University of Oklahoma, USA, 132 pp., 2017. <https://hdl.handle.net/11244/50907>

Zang, A., Oye, V., Jousset, P., Deichmann, N., Gritto, R., McGarr, A., Majer, E., and Bruhn, D., 2014. Analysis of induced seismicity in geothermal reservoirs–An overview. Geothermics, 52, pp.6-21. <https://doi.org/10.1016/j.geothermics.2014.06.005>

Zang, A., Stephansson, O., Stenberg, L., Plenkers, K., Specht, S., Milkereit, C., Schill, E., Kwiatek, G., Dresen, G., Zimmermann, G. and Dahm, T., 2017. Hydraulic fracture monitoring in hard rock at 410 m depth with an advanced fluid-injection protocol and extensive sensor array. Geophysical Journal International, 208(2), pp.790-813. <https://doi.org/10.1093/gji/ggw430>

Zang, A., Zimmermann, G., Hofmann, H., Stephansson, O., Min, K.B. and Kim, K.Y., 2019. How to reduce fluid-injection-induced seismicity. Rock Mechanics and Rock Engineering, 52(2), pp.475-493. <https://doi.org/10.1007/s00603-018-1467-4>

Zappone, A., Rinaldi, A.P., Grab, M., Wenning, Q.C., Roques, C., Madonna, C., Obermann, A.C., Bernasconi, S.M., Brennwald, M.S., Kipfer, R. and Soom, F., 2021. Fault sealing and caprock integrity for CO2 storage: an in situ injection experiment. Solid Earth, 12(2), pp.319-343. <https://doi.org/10.5194/se-12-319-2021>

Zbinden, D., Rinaldi, A.P., Diehl, T. and Wiemer, S., 2020. Hydromechanical modeling of fault reactivation in the St. Gallen deep geothermal project (Switzerland): poroelasticity or hydraulic connection?. Geophysical Research Letters, 47(3), p.e2019GL085201. <https://doi.org/10.1029/2019GL085201>

Zbinden, D., Rinaldi, A.P., Diehl, T. and Wiemer, S., 2020. Potential influence of overpressurized gas on the induced seismicity in the St. Gallen deep geothermal project (Switzerland). Solid Earth, 11(3), pp.909-933. <https://doi.org/10.5194/se-11-909-2020>

Zemach, E., Drakos, P., Spielman, P. and Akerley, J., 2013. Desert Peak East Enhanced Geothermal Systems (EGS) Project (No. DE-FC36-02ID14406). Ormat Technologies Inc., Reno, NV (United States).

Zhai, G., Shirzaei, M. and Manga, M., 2021. Widespread deep seismicity in the Delaware Basin, Texas, is mainly driven by shallow wastewater injection. Proceedings of the National Academy of Sciences, 118(20). <https://doi.org/10.1073/pnas.2102338118>

Zhai, G., Shirzaei, M., Manga, M., and Chen, X., 2019. Pore-pressure diffusion, enhanced by poroelastic stresses, controls induced seismicity in Oklahoma. Proceedings of the National Academy of Sciences, 116(33), pp.16228-16233. <https://doi.org/10.1073/pnas.1819225116>

Zhang, J., Zheng, H., Wang, G., Liu, Z., Qi, Y., Huang, Z. and Fan, X., 2020. In-situ stresses, abnormal pore pressures and their impacts on the Triassic Xujiahe reservoirs in tectonically active western Sichuan basin. Marine and Petroleum Geology, 122, p.104708. <https://doi.org/10.1016/j.marpetgeo.2020.104708>

Zhang, Y., 2003. Assessment of the Kaldárholt geothermal system and associated reinjection into the nearby Laugaland system, S-Iceland. UNU Geothermal Training Programme, Reports 2003, pp.527-552.

Zhang, Y., Person, M., Rupp, J., Ellett, K., Celia, M.A., Gable, C.W., Bowen, B., Evans, J., Bandilla, K., Mozley, P. and Dewers, T., 2013. Hydrogeologic controls on induced seismicity in crystalline basement rocks due to fluid injection into basal reservoirs. Groundwater, 51(4), pp.525-538. <https://doi.org/10.1111/gwat.12071>

Zhang, Y., Qiu, Z., Li, G., Zhong, H., Zhao, X., 2020. Analysis of interactions between water and shale by water activity. Journal of Natural Gas Science and Engineering 80, 103372. <https://doi.org/10.1016/j.jngse.2020.103372>

Zhao, B., 2018. Zhao, Bodi, "Geomechanical Modelling of Induced Seismicity" (2018). Electronic Thesis and Dissertation Repository. 5564. <https://ir.lib.uwo.ca/etd/5564>

Zheng, H., Zhang, J., Qi, Y., 2020. Geology and geomechanics of hydraulic fracturing in the Marcellus shale gas play and their potential applications to the Fuling shale gas development. Energy Geoscience 1, 36–46. <https://doi.org/10.1016/j.engeos.2020.05.002>

Zheng, M., Tang, H., Li, H., Zheng, J. and Jing, C., 2020. Geomechanical Analysis for Deep Shale Gas Exploration Wells in the NDNR Blocks, Sichuan Basin, Southwest China. Energies, 13(5), p.1117. <https://doi.org/10.3390/en13051117>

Ziegler, M. and Evans, K.F., 2020. Comparative study of Basel EGS reservoir faults inferred from analysis of microseismic cluster datasets with fracture zones obtained from well log analysis. Journal of Structural Geology, 130, p.103923. <https://doi.org/10.1016/j.jsg.2019.103923>

Ziegler, M., Rajabi, M., Heidbach, O., Hersir, G.P., Ágústsson, K., Árnadóttir, S. and Zang, A., 2016. The stress pattern of Iceland. Tectonophysics, 674, pp.101-113. <https://doi.org/10.1016/j.tecto.2016.02.008>

Zielke, O., Arrowsmith, J. R., Grant Ludwig, L., and Akciz, S. O., 2012. High‐resolution topography‐derived offsets along the 1857 Fort Tejon earthquake rupture trace, San Andreas fault. Bulletin of the Seismological Society of America, 102(3), pp.1135-1154. <https://doi.org/10.1785/0120110230>

Zoback, M.D. and Harjes, H.P., 1997. Injection‐induced earthquakes and crustal stress at 9 km depth at the KTB deep drilling site, Germany. Journal of Geophysical Research: Solid Earth, 102(B8), pp.18477-18491. <https://doi.org/10.1029/96JB02814>

Zúñiga, F.R., Castro, R.R. and Dominguez, T., 1995. Stress orientation and anisotropy based on shear-wave splitting observations in the Cerro Prieto fault area, Baja California, Mexico. pure and applied geophysics, 144(1), pp.39-57. <https://doi.org/10.1007/BF00876473>